(footprint "Molex_Mini-Fit_Sr_42820-22XX_1x02_P10.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Mini-Fit Sr. Power Connectors, 42820-22XX, 2 Pins per row (http://www.molex.com/pdm_docs/sd/428202214_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Mini-Fit_Sr top entry")
	(property "Reference" "REF**"
		(at 17.06 -8.93 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Mini-Fit_Sr_42820-22XX_1x02_P10.00mm_Horizontal"
		(at 17.06 18.93 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 17.06 14.75 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 14 -5.73)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 14 15.73)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 5.1 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 5 0)
		(size 5.1 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 0 10)
		(size 5.1 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 5 10)
		(size 5.1 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Sr_42820-22XX_1x02_P10.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
