(footprint "Molex_Mini-Fit_Sr_43915-xx12_2x06_P10.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Mini-Fit Sr. Power Connectors, 43915-xx12, 6 Pins per row (http://www.molex.com/pdm_docs/sd/439151404_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Mini-Fit_Sr side entry")
	(property "Reference" "REF**"
		(at 8.43 -11.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Mini-Fit_Sr_43915-xx12_2x06_P10.00mm_Vertical"
		(at 8.43 61.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8.43 54.75 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at 8.43 -5.705)
		(size 3.5 3.5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" np_thru_hole circle
		(at 8.43 5)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" thru_hole circle
		(at 8.43 55.705)
		(size 3.5 3.5)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 4.4 0)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 0 10)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 4.4 10)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 0 20)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 4.4 20)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole rect
		(at 0 30)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole rect
		(at 4.4 30)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole rect
		(at 0 40)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole rect
		(at 4.4 40)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole rect
		(at 0 50)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole rect
		(at 4.4 50)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole rect
		(at 12.46 0)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole rect
		(at 16.86 0)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole rect
		(at 12.46 10)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole rect
		(at 16.86 10)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole rect
		(at 12.46 20)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole rect
		(at 16.86 20)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole rect
		(at 12.46 30)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole rect
		(at 16.86 30)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole rect
		(at 12.46 40)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole rect
		(at 16.86 40)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole rect
		(at 12.46 50)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole rect
		(at 16.86 50)
		(size 4.5 4.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Mini-Fit_Sr_43915-xx12_2x06_P10.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
