(footprint "Molex_Nano-Fit_105309-xx02_1x02_P2.50mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Nano-Fit Power Connectors, 105309-xx02, 2 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Nano-Fit side entry")
	(property "Reference" "REF**"
		(at 0 -2.92 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Nano-Fit_105309-xx02_1x02_P2.50mm_Vertical"
		(at 0 5.42 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.1 1.25 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.34 1.25)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole custom
		(at 0 0)
		(size 1.417157 1.417157)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.85 0.6) (xy -0.45 0.6) (xy -0.85 0.2) (xy -0.85 -0.6) (xy 0.85 -0.6)
				)
				(width 0.5)
				(fill yes)
			)
		)
	)
	(pad "2" thru_hole oval
		(at 0 2.5)
		(size 2.2 1.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx02_1x02_P2.50mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
