(footprint "Molex_Pico-SPOX_87437-1443_1x14-P1.5mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Pico-SPOX Connector System, 87437-1443, 14 Pins per row (https://www.molex.com/pdm_docs/sd/874371443_sd.pdf#page=2)")
	(tags "molex pico spox 14")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Pico-SPOX_87437-1443_1x14-P1.5mm_Vertical"
		(at 0 5.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -9.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.25 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.25 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.25 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.25 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.25 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.25 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.25 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.25 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 5.25 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 5.25 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 6.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 6.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 8.25 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 8.25 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 9.75 -2.175 90)
		(size 2.65 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 9.75 1.725 90)
		(size 3.55 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Pico-SPOX_87437-1443_1x14-P1.5mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
