(footprint "Molex_PicoBlade_53398-0471_1x04-1MP_P1.25mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex PicoBlade series connector, 53398-0471 (http://www.molex.com/pdm_docs/sd/533980271_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex PicoBlade side entry")
	(property "Reference" "REF**"
		(at 0 -3.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_PicoBlade_53398-0471_1x04-1MP_P1.25mm_Vertical"
		(at 0 4.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.4 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.875 -1.25)
		(size 0.8 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.625 -1.25)
		(size 0.8 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.625 -1.25)
		(size 0.8 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 1.875 -1.25)
		(size 0.8 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -4.425 1.5)
		(size 2.1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.119048)
	)
	(pad "MP" smd roundrect
		(at 4.425 1.5)
		(size 2.1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.119048)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_PicoBlade_53398-0471_1x04-1MP_P1.25mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
