(footprint "Molex_Picoflex_90814-0004_2x02_P1.27mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Picoflex Ribbon-Cable Connectors, 90814-0004, 4 Pins (http://www.molex.com/pdm_docs/sd/908140004_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Picoflex side entry")
	(property "Reference" "REF**"
		(at 0 -6.16 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Picoflex_90814-0004_2x02_P1.27mm_Vertical"
		(at 0 6.16 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEPOUT"
		(at 0 0 90)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at -1.35 0 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.9 -3.83)
		(size 1.9 1.9)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.9 3.83)
		(size 1.9 1.9)
		(drill 1.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -3 -1.91)
		(size 2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3 -0.64)
		(size 2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3 0.63)
		(size 2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3 1.9)
		(size 2 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Picoflex_90814-0004_2x02_P1.27mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
