(footprint "Molex_SL_171971-0025_1x25_P2.54mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Stackable Linear Connector, 171971-0025 (compatible alternatives: 171971-0125, 171971-0225), 25 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex SL vertical")
	(property "Reference" "REF**"
		(at 30.48 -3.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_SL_171971-0025_1x25_P2.54mm_Vertical"
		(at 30.48 5.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 30.48 1.85 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.143678)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 5.08 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 7.62 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 10.16 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 12.7 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 15.24 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 17.78 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 20.32 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 22.86 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 25.4 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 27.94 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 30.48 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 33.02 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 35.56 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 38.1 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 40.64 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 43.18 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 45.72 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 48.26 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 50.8 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 53.34 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 55.88 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 58.42 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 60.96 0)
		(size 1.74 1.74)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0025_1x25_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
