(footprint "Molex_Sabre_43160-1103_1x03_P7.49mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Sabre Power Connector, 43160-1103, 3 Pins per row (http://www.molex.com/pdm_docs/sd/431605304_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Sabre top entry")
	(property "Reference" "REF**"
		(at 7.49 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Sabre_43160-1103_1x03_P7.49mm_Horizontal"
		(at 7.49 16.89 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.49 14.98 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -4.75 13.13)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 19.73 13.13)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 7.49 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 7.49 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 14.98 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 14.98 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Sabre_43160-1103_1x03_P7.49mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
