(footprint "Molex_Sabre_43160-2106_1x06_P7.49mm_Vertical_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex Sabre Power Connector, 43160-2106, With thermal vias in pads, 6 Pins per row (http://www.molex.com/pdm_docs/sd/431602102_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Sabre side entry")
	(property "Reference" "REF**"
		(at 18.72 -10.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Sabre_43160-2106_1x06_P7.49mm_Vertical_ThermalVias"
		(at 18.72 5.08 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 18.72 3.18 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -4.75 -3.43)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 42.2 -3.43)
		(size 4 4)
		(drill 3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at -1.44 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at -1.44 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at -1.44 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at -1.44 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at -1.44 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 1.44 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 1.44 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 1.44 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 1.44 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 1.44 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.05 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.05 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.05 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.05 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.05 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.49 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 7.49 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.49 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 7.49 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.49 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 8.93 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 8.93 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 8.93 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 8.93 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 8.93 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 13.54 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 13.54 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 13.54 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 13.54 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 13.54 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 14.98 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 14.98 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 14.98 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 14.98 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 14.98 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 16.42 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 16.42 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 16.42 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 16.42 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 16.42 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 21.03 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 21.03 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 21.03 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 21.03 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 21.03 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 22.47 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole rect
		(at 22.47 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 22.47 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole rect
		(at 22.47 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 22.47 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 23.91 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 23.91 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 23.91 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 23.91 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 23.91 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 28.52 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 28.52 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 28.52 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 28.52 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 28.52 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 29.96 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole rect
		(at 29.96 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 29.96 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole rect
		(at 29.96 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 29.96 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 31.4 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 31.4 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 31.4 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 31.4 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 31.4 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 36.01 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 36.01 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 36.01 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 36.01 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 36.01 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 37.45 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole rect
		(at 37.45 -3.18)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 37.45 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole rect
		(at 37.45 0)
		(size 3.78 3.43)
		(drill 1.78)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 37.45 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 38.89 -4.445)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 38.89 -3.0175)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 38.89 -1.59)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 38.89 -0.1625)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 38.89 1.265)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Sabre_43160-2106_1x06_P7.49mm_Vertical_ThermalVias.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
