(footprint "BUS_AT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AT ISA 16 bits Bus Edge Connector")
	(tags "BUS ISA AT Edge connector")
	(property "Reference" "REF**"
		(at -60.96 -6.99 0)
		(layer "F.SilkS")
	)
	(property "Value" "BUS_AT"
		(at -81.91 -6.99 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at -64.77 -0.635 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at 0 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "2" connect rect
		(at -2.54 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -5.08 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "4" connect rect
		(at -7.62 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -10.16 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "6" connect rect
		(at -12.7 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -15.24 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "8" connect rect
		(at -17.78 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at -20.32 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "10" connect rect
		(at -22.86 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at -25.4 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "12" connect rect
		(at -27.94 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at -30.48 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "14" connect rect
		(at -33.02 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at -35.56 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "16" connect rect
		(at -38.1 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at -40.64 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "18" connect rect
		(at -43.18 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at -45.72 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "20" connect rect
		(at -48.26 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at -50.8 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "22" connect rect
		(at -53.34 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at -55.88 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "24" connect rect
		(at -58.42 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at -60.96 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "26" connect rect
		(at -63.5 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at -66.04 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "28" connect rect
		(at -68.58 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at -71.12 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "30" connect rect
		(at -73.66 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at -76.2 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "32" connect rect
		(at 0 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "33" connect rect
		(at -2.54 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at -5.08 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "35" connect rect
		(at -7.62 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at -10.16 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "37" connect rect
		(at -12.7 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at -15.24 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" connect rect
		(at -17.78 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at -20.32 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "41" connect rect
		(at -22.86 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at -25.4 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "43" connect rect
		(at -27.94 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at -30.48 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "45" connect rect
		(at -33.02 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at -35.56 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "47" connect rect
		(at -38.1 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at -40.64 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "49" connect rect
		(at -43.18 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at -45.72 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "51" connect rect
		(at -48.26 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" connect rect
		(at -50.8 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "53" connect rect
		(at -53.34 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" connect rect
		(at -55.88 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "55" connect rect
		(at -58.42 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" connect rect
		(at -60.96 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "57" connect rect
		(at -63.5 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" connect rect
		(at -66.04 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "59" connect rect
		(at -68.58 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" connect rect
		(at -71.12 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "61" connect rect
		(at -73.66 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" connect rect
		(at -76.2 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "63" connect rect
		(at -86.36 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "64" connect rect
		(at -88.9 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "65" connect rect
		(at -91.44 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "66" connect rect
		(at -93.98 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "67" connect rect
		(at -96.52 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "68" connect rect
		(at -99.06 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "69" connect rect
		(at -101.6 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "70" connect rect
		(at -104.14 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "71" connect rect
		(at -106.68 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "72" connect rect
		(at -109.22 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "73" connect rect
		(at -111.76 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "74" connect rect
		(at -114.3 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "75" connect rect
		(at -116.84 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "76" connect rect
		(at -119.38 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "77" connect rect
		(at -121.92 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "78" connect rect
		(at -124.46 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "79" connect rect
		(at -127 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "80" connect rect
		(at -129.54 0)
		(size 1.78 7.62)
		(layers "B.Cu" "B.Mask")
	)
	(pad "81" connect rect
		(at -86.36 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "82" connect rect
		(at -88.9 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "83" connect rect
		(at -91.44 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "84" connect rect
		(at -93.98 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "85" connect rect
		(at -96.52 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "86" connect rect
		(at -99.06 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "87" connect rect
		(at -101.6 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "88" connect rect
		(at -104.14 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "89" connect rect
		(at -106.68 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "90" connect rect
		(at -109.22 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "91" connect rect
		(at -111.76 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "92" connect rect
		(at -114.3 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "93" connect rect
		(at -116.84 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "94" connect rect
		(at -119.38 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "95" connect rect
		(at -121.92 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "96" connect rect
		(at -124.46 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "97" connect rect
		(at -127 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(pad "98" connect rect
		(at -129.54 0)
		(size 1.78 7.62)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
