(footprint "BUS_PCI_Express_Mini_Dual"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mini-PCI Express bus connector full size with dual clips (https://s3.amazonaws.com/fit-iot/download/facet-cards/documents/PCI_Express_miniCard_Electromechanical_specs_rev1.2.pdf#page=28)")
	(tags "mini pcie")
	(property "Reference" "REF**"
		(at -12.5 6.35 180)
		(layer "F.SilkS")
	)
	(property "Value" "BUS_PCI_Express_Mini_Dual"
		(at 0 6.35 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -12.5 0)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.5 0)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -11.8 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -11.4 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -11 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -10.6 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -10.2 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -9.8 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -9.4 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -9 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8.6 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -8.2 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -7.8 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -7.4 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -7 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -6.6 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -6.2 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -5.8 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -2.2 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.8 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.4 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -1 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -0.6 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -0.2 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.2 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0.6 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.4 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 1.8 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 2.2 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.6 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.4 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.8 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 4.2 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 4.6 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 5 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 5.4 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 5.8 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 6.2 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 6.6 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 7 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 7.4 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 7.8 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 8.2 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 8.6 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 9 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 9.4 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 9.8 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 10.2 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 10.6 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 11 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 11.4 4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 11.8 -4.1)
		(size 0.6 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -14.65 3.5)
		(size 2.3 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 14.65 3.5)
		(size 2.3 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/BUS_PCI_Express_Mini_Dual.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
