(footprint "BUS_PCIexpress_x1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PCIexpress Bus Edge Connector x1 http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=70")
	(tags "PCIe")
	(property "Reference" "REF**"
		(at 5 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BUS_PCIexpress_x1"
		(at 10.33 -8.01 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -0.65 -4.95)
		(end -0.65 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.65 2.95)
		(end -0.15 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.15 3.45)
		(end 10.05 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.55 -4)
		(end 10.55 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.55 2.95)
		(end 10.05 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.45 -4)
		(end 12.45 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.45 2.95)
		(end 12.95 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.95 3.45)
		(end 19.15 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 19.65 -4.95)
		(end 19.65 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 19.65 2.95)
		(end 19.15 3.45)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 10.55 -4)
		(mid 11.5 -4.95)
		(end 12.45 -4)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB Thickness 1.57 mm"
		(at 5 2.8 180)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 16 -3.5 0)
		(layer "F.Fab")
	)
	(pad "A1" connect rect
		(at 0 -0.55)
		(size 0.7 3.2)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A2" connect rect
		(at 1 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A3" connect rect
		(at 2 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A4" connect rect
		(at 3 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A5" connect rect
		(at 4 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A6" connect rect
		(at 5 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A7" connect rect
		(at 6 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A8" connect rect
		(at 7 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A9" connect rect
		(at 8 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A10" connect rect
		(at 9 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A11" connect rect
		(at 10 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A12" connect rect
		(at 13 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A13" connect rect
		(at 14 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A14" connect rect
		(at 15 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A15" connect rect
		(at 16 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A16" connect rect
		(at 17 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A17" connect rect
		(at 18 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A18" connect rect
		(at 19 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "B1" connect rect
		(at 0 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" connect rect
		(at 1 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" connect rect
		(at 2 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" connect rect
		(at 3 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B5" connect rect
		(at 4 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B6" connect rect
		(at 5 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B7" connect rect
		(at 6 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B8" connect rect
		(at 7 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B9" connect rect
		(at 8 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B10" connect rect
		(at 9 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B11" connect rect
		(at 10 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B12" connect rect
		(at 13 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B13" connect rect
		(at 14 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B14" connect rect
		(at 15 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B15" connect rect
		(at 16 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B16" connect rect
		(at 17 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B17" connect rect
		(at 18 -0.55)
		(size 0.7 3.2)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B18" connect rect
		(at 19 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
