(footprint "BUS_PCIexpress_x16"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PCIexpress Bus Edge Connector x1 http://www.ritrontek.com/uploadfile/2016/1026/20161026105231124.pdf#page=70")
	(tags "PCIe")
	(property "Reference" "REF**"
		(at 5 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BUS_PCIexpress_x16"
		(at 10.33 -8.01 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -0.65 -4.95)
		(end -0.65 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.65 2.95)
		(end -0.15 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.15 3.45)
		(end 10.05 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.55 -4)
		(end 10.55 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.55 2.95)
		(end 10.05 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.45 -4)
		(end 12.45 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.45 2.95)
		(end 12.95 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.95 3.45)
		(end 83.15 3.45)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 83.65 -4.95)
		(end 83.65 2.95)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 83.65 2.95)
		(end 83.15 3.45)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 10.55 -4)
		(mid 11.5 -4.95)
		(end 12.45 -4)
		(layer "Edge.Cuts")
	)
	(fp_text user "PCB Thickness 1.57 mm"
		(at 5 2.8 180)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 16 -3.5 0)
		(layer "F.Fab")
	)
	(pad "A1" connect rect
		(at 0 -0.55)
		(size 0.7 3.2)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A2" connect rect
		(at 1 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A3" connect rect
		(at 2 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A4" connect rect
		(at 3 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A5" connect rect
		(at 4 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A6" connect rect
		(at 5 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A7" connect rect
		(at 6 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A8" connect rect
		(at 7 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A9" connect rect
		(at 8 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A10" connect rect
		(at 9 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A11" connect rect
		(at 10 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A12" connect rect
		(at 13 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A13" connect rect
		(at 14 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A14" connect rect
		(at 15 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A15" connect rect
		(at 16 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A16" connect rect
		(at 17 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A17" connect rect
		(at 18 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A18" connect rect
		(at 19 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A19" connect rect
		(at 20 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A20" connect rect
		(at 21 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A21" connect rect
		(at 22 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A22" connect rect
		(at 23 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A23" connect rect
		(at 24 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A24" connect rect
		(at 25 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A25" connect rect
		(at 26 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A26" connect rect
		(at 27 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A27" connect rect
		(at 28 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A28" connect rect
		(at 29 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A29" connect rect
		(at 30 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A30" connect rect
		(at 31 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A31" connect rect
		(at 32 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A32" connect rect
		(at 33 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A33" connect rect
		(at 34 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A34" connect rect
		(at 35 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A35" connect rect
		(at 36 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A36" connect rect
		(at 37 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A37" connect rect
		(at 38 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A38" connect rect
		(at 39 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A39" connect rect
		(at 40 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A40" connect rect
		(at 41 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A41" connect rect
		(at 42 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A42" connect rect
		(at 43 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A43" connect rect
		(at 44 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A44" connect rect
		(at 45 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A45" connect rect
		(at 46 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A46" connect rect
		(at 47 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A47" connect rect
		(at 48 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A48" connect rect
		(at 49 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A49" connect rect
		(at 50 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A50" connect rect
		(at 51 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A51" connect rect
		(at 52 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A52" connect rect
		(at 53 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A53" connect rect
		(at 54 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A54" connect rect
		(at 55 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A55" connect rect
		(at 56 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A56" connect rect
		(at 57 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A57" connect rect
		(at 58 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A58" connect rect
		(at 59 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A59" connect rect
		(at 60 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A60" connect rect
		(at 61 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A61" connect rect
		(at 62 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A62" connect rect
		(at 63 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A63" connect rect
		(at 64 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A64" connect rect
		(at 65 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A65" connect rect
		(at 66 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A66" connect rect
		(at 67 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A67" connect rect
		(at 68 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A68" connect rect
		(at 69 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A69" connect rect
		(at 70 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A70" connect rect
		(at 71 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A71" connect rect
		(at 72 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A72" connect rect
		(at 73 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A73" connect rect
		(at 74 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A74" connect rect
		(at 75 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A75" connect rect
		(at 76 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A76" connect rect
		(at 77 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A77" connect rect
		(at 78 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A78" connect rect
		(at 79 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A79" connect rect
		(at 80 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A80" connect rect
		(at 81 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A81" connect rect
		(at 82 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A82" connect rect
		(at 83 0)
		(size 0.7 4.3)
		(layers "B.Cu" "B.Mask")
	)
	(pad "B1" connect rect
		(at 0 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" connect rect
		(at 1 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" connect rect
		(at 2 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" connect rect
		(at 3 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B5" connect rect
		(at 4 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B6" connect rect
		(at 5 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B7" connect rect
		(at 6 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B8" connect rect
		(at 7 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B9" connect rect
		(at 8 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B10" connect rect
		(at 9 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B11" connect rect
		(at 10 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B12" connect rect
		(at 13 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B13" connect rect
		(at 14 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B14" connect rect
		(at 15 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B15" connect rect
		(at 16 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B16" connect rect
		(at 17 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B17" connect rect
		(at 18 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B18" connect rect
		(at 19 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B19" connect rect
		(at 20 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B20" connect rect
		(at 21 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B21" connect rect
		(at 22 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B22" connect rect
		(at 23 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B23" connect rect
		(at 24 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B24" connect rect
		(at 25 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B25" connect rect
		(at 26 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B26" connect rect
		(at 27 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B27" connect rect
		(at 28 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B28" connect rect
		(at 29 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B29" connect rect
		(at 30 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B30" connect rect
		(at 31 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B31" connect rect
		(at 32 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B32" connect rect
		(at 33 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B33" connect rect
		(at 34 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B34" connect rect
		(at 35 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B35" connect rect
		(at 36 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B36" connect rect
		(at 37 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B37" connect rect
		(at 38 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B38" connect rect
		(at 39 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B39" connect rect
		(at 40 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B40" connect rect
		(at 41 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B41" connect rect
		(at 42 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B42" connect rect
		(at 43 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B43" connect rect
		(at 44 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B44" connect rect
		(at 45 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B45" connect rect
		(at 46 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B46" connect rect
		(at 47 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B47" connect rect
		(at 48 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B48" connect rect
		(at 49 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B49" connect rect
		(at 50 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B50" connect rect
		(at 51 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B51" connect rect
		(at 52 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B52" connect rect
		(at 53 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B53" connect rect
		(at 54 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B54" connect rect
		(at 55 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B55" connect rect
		(at 56 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B56" connect rect
		(at 57 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B57" connect rect
		(at 58 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B58" connect rect
		(at 59 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B59" connect rect
		(at 60 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B60" connect rect
		(at 61 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B61" connect rect
		(at 62 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B62" connect rect
		(at 63 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B63" connect rect
		(at 64 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B64" connect rect
		(at 65 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B65" connect rect
		(at 66 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B66" connect rect
		(at 67 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B67" connect rect
		(at 68 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B68" connect rect
		(at 69 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B69" connect rect
		(at 70 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B70" connect rect
		(at 71 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B71" connect rect
		(at 72 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B72" connect rect
		(at 73 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B73" connect rect
		(at 74 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B74" connect rect
		(at 75 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B75" connect rect
		(at 76 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B76" connect rect
		(at 77 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B77" connect rect
		(at 78 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B78" connect rect
		(at 79 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B79" connect rect
		(at 80 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B80" connect rect
		(at 81 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B81" connect rect
		(at 82 -0.55)
		(size 0.7 3.2)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B82" connect rect
		(at 83 0)
		(size 0.7 4.3)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
