(footprint "JAE_MM60-EZH039-Bx_BUS_PCI_Express_Holder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PCI Express mini card latch for 3.9mm connector height, https://www.jae.com/direct/topics/topics_file_download/?topics_id=68909&ext_no=06&index=0&_lang=en&v=2022071912512930114109")
	(tags "MiniPCI")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "JAE_MM60-EZH039-Bx_BUS_PCI_Express_Holder"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -12.1 2.3)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.1 2.3)
		(size 1.05 1.05)
		(drill 1.05)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "MP" smd roundrect
		(at -13.35 5.45)
		(size 1.2 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "MP" smd roundrect
		(at -12.1 -0.45)
		(size 1.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "MP" smd roundrect
		(at -10.85 5.45)
		(size 1.2 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "MP" smd roundrect
		(at 10.85 5.45)
		(size 1.2 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(pad "MP" smd roundrect
		(at 12.1 -0.45)
		(size 1.5 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "MP" smd roundrect
		(at 13.35 5.45)
		(size 1.2 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2083333333)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/JAE_MM60-EZH039-Bx_BUS_PCI_Express_Holder.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
