(footprint "SODIMM-200_1.8V_Card_edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SODIMM 200-pins edge connector, Jedec MO-224 Variation AB compliant (1.8V DDR2 SDRAM), 0.6mm pitch, https://www.jst-mfg.com/product/pdf/eng/eDM-200P.pdf")
	(tags "sodimm")
	(property "Reference" "REF**"
		(at 2.895 -3.235 0)
		(layer "F.SilkS")
	)
	(property "Value" "SODIMM-200_1.8V_Card_edge"
		(at 32.125 2.375 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
	(fp_line
		(start -2.15 -20.625)
		(end -2.15 -24.025)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.15 1.375)
		(end -2.15 -16.625)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 13.6 1.375)
		(end -2.15 1.375)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 13.6 1.375)
		(end 13.6 -2.125)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.6 -2.125)
		(end 14.6 1.375)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.6 1.375)
		(end 65.45 1.375)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 65.45 -20.625)
		(end 65.45 -24.025)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 65.45 1.375)
		(end 65.45 -16.625)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -2.15 -20.625)
		(mid -0.15 -18.625)
		(end -2.15 -16.625)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 13.6 -2.125)
		(mid 14.1 -2.625)
		(end 14.6 -2.125)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 65.45 -16.625)
		(mid 63.45 -18.625)
		(end 65.45 -20.625)
		(layer "Edge.Cuts")
	)
	(fp_text user "< 0.2mm"
		(at 13.8 7.825 180)
		(layer "Cmts.User")
	)
	(fp_text user "< 0.2mm"
		(at 13.8 10.325 180)
		(layer "Cmts.User")
	)
	(fp_text user "Optional hole 1.8mm diam"
		(at 66.15 -4.53 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Optional PCB chamfer setback:"
		(at 19.16 6.51 180)
		(layer "Cmts.User")
	)
	(fp_text user "PCB connector edge"
		(at 21.9 9.125 180)
		(layer "Cmts.User")
	)
	(fp_text user "PCB Thickness 1 mm"
		(at 3.74 2.105 180)
		(layer "Cmts.User")
	)
	(fp_text user "Optional hole 1.8 diam mm"
		(at -3.02 -5.02 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "< 0.2mm"
		(at 18.2 12.825 180)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 31.65 0.075 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at 0 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at 0.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at 0.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at 0.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at 1.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at 1.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at 1.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at 2.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at 2.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at 2.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at 3 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at 3.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at 3.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at 3.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at 4.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at 4.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at 4.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at 5.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at 5.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" connect rect
		(at 5.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at 6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" connect rect
		(at 6.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at 6.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" connect rect
		(at 6.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at 7.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" connect rect
		(at 7.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at 7.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" connect rect
		(at 8.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at 8.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" connect rect
		(at 8.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at 9 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" connect rect
		(at 9.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "33" connect rect
		(at 9.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at 9.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "35" connect rect
		(at 10.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at 10.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "37" connect rect
		(at 10.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at 11.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "39" connect rect
		(at 11.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at 11.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "41" connect rect
		(at 15.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at 15.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "43" connect rect
		(at 16.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at 16.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "45" connect rect
		(at 16.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at 17.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "47" connect rect
		(at 17.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at 17.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "49" connect rect
		(at 18 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at 18.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "51" connect rect
		(at 18.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" connect rect
		(at 18.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "53" connect rect
		(at 19.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" connect rect
		(at 19.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "55" connect rect
		(at 19.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" connect rect
		(at 20.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "57" connect rect
		(at 20.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" connect rect
		(at 20.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "59" connect rect
		(at 21 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" connect rect
		(at 21.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "61" connect rect
		(at 21.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" connect rect
		(at 21.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "63" connect rect
		(at 22.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "64" connect rect
		(at 22.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "65" connect rect
		(at 22.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "66" connect rect
		(at 23.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "67" connect rect
		(at 23.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "68" connect rect
		(at 23.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "69" connect rect
		(at 24 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "70" connect rect
		(at 24.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "71" connect rect
		(at 24.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "72" connect rect
		(at 24.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "73" connect rect
		(at 25.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "74" connect rect
		(at 25.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "75" connect rect
		(at 25.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "76" connect rect
		(at 26.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "77" connect rect
		(at 26.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "78" connect rect
		(at 26.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "79" connect rect
		(at 27 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "80" connect rect
		(at 27.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "81" connect rect
		(at 27.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "82" connect rect
		(at 27.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "83" connect rect
		(at 28.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "84" connect rect
		(at 28.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "85" connect rect
		(at 28.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "86" connect rect
		(at 29.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "87" connect rect
		(at 29.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "88" connect rect
		(at 29.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "89" connect rect
		(at 30 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "90" connect rect
		(at 30.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "91" connect rect
		(at 30.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "92" connect rect
		(at 30.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "93" connect rect
		(at 31.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "94" connect rect
		(at 31.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "95" connect rect
		(at 31.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "96" connect rect
		(at 32.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "97" connect rect
		(at 32.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "98" connect rect
		(at 32.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "99" connect rect
		(at 33 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "100" connect rect
		(at 33.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "101" connect rect
		(at 33.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "102" connect rect
		(at 33.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "103" connect rect
		(at 34.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "104" connect rect
		(at 34.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "105" connect rect
		(at 34.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "106" connect rect
		(at 35.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "107" connect rect
		(at 35.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "108" connect rect
		(at 35.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "109" connect rect
		(at 36 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "110" connect rect
		(at 36.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "111" connect rect
		(at 36.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "112" connect rect
		(at 36.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "113" connect rect
		(at 37.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "114" connect rect
		(at 37.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "115" connect rect
		(at 37.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "116" connect rect
		(at 38.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "117" connect rect
		(at 38.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "118" connect rect
		(at 38.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "119" connect rect
		(at 39 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "120" connect rect
		(at 39.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "121" connect rect
		(at 39.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "122" connect rect
		(at 39.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "123" connect rect
		(at 40.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "124" connect rect
		(at 40.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "125" connect rect
		(at 40.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "126" connect rect
		(at 41.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "127" connect rect
		(at 41.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "128" connect rect
		(at 41.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "129" connect rect
		(at 42 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "130" connect rect
		(at 42.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "131" connect rect
		(at 42.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "132" connect rect
		(at 42.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "133" connect rect
		(at 43.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "134" connect rect
		(at 43.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "135" connect rect
		(at 43.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "136" connect rect
		(at 44.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "137" connect rect
		(at 44.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "138" connect rect
		(at 44.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "139" connect rect
		(at 45 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "140" connect rect
		(at 45.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "141" connect rect
		(at 45.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "142" connect rect
		(at 45.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "143" connect rect
		(at 46.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "144" connect rect
		(at 46.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "145" connect rect
		(at 46.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "146" connect rect
		(at 47.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "147" connect rect
		(at 47.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "148" connect rect
		(at 47.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "149" connect rect
		(at 48 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "150" connect rect
		(at 48.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "151" connect rect
		(at 48.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "152" connect rect
		(at 48.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "153" connect rect
		(at 49.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "154" connect rect
		(at 49.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "155" connect rect
		(at 49.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "156" connect rect
		(at 50.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "157" connect rect
		(at 50.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "158" connect rect
		(at 50.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "159" connect rect
		(at 51 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "160" connect rect
		(at 51.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "161" connect rect
		(at 51.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "162" connect rect
		(at 51.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "163" connect rect
		(at 52.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "164" connect rect
		(at 52.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "165" connect rect
		(at 52.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "166" connect rect
		(at 53.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "167" connect rect
		(at 53.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "168" connect rect
		(at 53.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "169" connect rect
		(at 54 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "170" connect rect
		(at 54.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "171" connect rect
		(at 54.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "172" connect rect
		(at 54.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "173" connect rect
		(at 55.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "174" connect rect
		(at 55.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "175" connect rect
		(at 55.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "176" connect rect
		(at 56.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "177" connect rect
		(at 56.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "178" connect rect
		(at 56.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "179" connect rect
		(at 57 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "180" connect rect
		(at 57.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "181" connect rect
		(at 57.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "182" connect rect
		(at 57.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "183" connect rect
		(at 58.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "184" connect rect
		(at 58.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "185" connect rect
		(at 58.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "186" connect rect
		(at 59.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "187" connect rect
		(at 59.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "188" connect rect
		(at 59.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "189" connect rect
		(at 60 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "190" connect rect
		(at 60.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "191" connect rect
		(at 60.6 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "192" connect rect
		(at 60.9 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "193" connect rect
		(at 61.2 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "194" connect rect
		(at 61.5 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "195" connect rect
		(at 61.8 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "196" connect rect
		(at 62.1 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "197" connect rect
		(at 62.4 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "198" connect rect
		(at 62.7 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(pad "199" connect rect
		(at 63 0)
		(size 0.45 2.35)
		(layers "F.Cu" "F.Mask")
	)
	(pad "200" connect rect
		(at 63.3 0)
		(size 0.45 2.35)
		(layers "B.Cu" "B.Mask")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.15 -12.6) (xy -0.15 -12.6) (xy -0.15 -18.625) (xy -2.15 -18.625)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.15 -1.175) (xy -0.275 -1.175) (xy -0.275 1.375) (xy -2.15 1.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.15 1.375) (xy -1.15 1.375) (xy -1.15 -12.6) (xy -2.15 -12.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 11.975 -1.175) (xy 15.35 -1.175) (xy 15.35 1.375) (xy 11.975 1.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 63.45 -12.6) (xy 65.45 -12.6) (xy 65.45 -18.625) (xy 63.45 -18.625)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 63.575 -1.175) (xy 65.45 -1.175) (xy 65.45 1.375) (xy 63.575 1.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64.45 1.375) (xy 65.45 1.375) (xy 65.45 -12.6) (xy 64.45 -12.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
			"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
			"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
			"In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.15 -16.125) (xy -0.15 -16.125) (xy -0.15 -18.625) (xy -2.15 -18.625)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
			"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
			"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
			"In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.15 1.375) (xy -2.15 0.375) (xy 65.45 0.375) (xy 65.45 1.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
			"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
			"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
			"In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.15 1.375) (xy -1.65 1.375) (xy -1.65 -16.125) (xy -2.15 -16.125)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
			"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
			"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
			"In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 63.45 -16.125) (xy 65.45 -16.125) (xy 65.45 -18.625) (xy 63.45 -18.625)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu" "In7.Cu"
			"In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu" "In15.Cu"
			"In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu" "In22.Cu"
			"In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu" "In29.Cu"
			"In30.Cu"
		)
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64.95 1.375) (xy 65.45 1.375) (xy 65.45 -16.125) (xy 64.95 -16.125)
			)
		)
	)
	(embedded_fonts no)
)
