(footprint "SODIMM-260_DDR4_H4.0-5.2_OrientationStd_Socket"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DDR4 SODIMM Socket, 0.5 mm pitch, 260 positions, 4 mm or 5 mm height, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F2309407%7F3%7Fpdf%7FEnglish%7FENG_CD_2309407_3.pdf%7F2309407-1")
	(tags "SODIMM DIMM DDR DDR4 RAM")
	(property "Reference" "REF**"
		(at -7.925 -37.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SODIMM-260_DDR4_H4.0-5.2_OrientationStd_Socket"
		(at 1.575 39.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "SODIMM MODULE OVER THIS AREA"
		(at 13.575 0 270)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 1.575 37.625 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -7.925 -34.4 270)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.925 34.4 270)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -12.025 -33.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.825001 -33.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -12.025 -32.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.825001 -32.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -12.025 -32.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.825001 -32.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -12.025 -31.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.825001 -31.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -12.025 -31.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.825001 -31.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -12.025 -30.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.825001 -30.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -12.025 -30.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.825001 -30.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -12.025 -29.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -3.825001 -29.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -12.025 -29.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -3.825001 -29.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -12.025 -28.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -3.825001 -28.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -12.025 -28.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -3.825001 -28.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -12.025 -27.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -3.825001 -27.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at -12.025 -27.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -3.825001 -27.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -12.025 -26.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -3.825001 -26.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at -12.025 -26.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at -3.825001 -26.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at -12.025 -25.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at -3.825001 -25.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at -12.025 -25.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at -3.825001 -25.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -12.025 -24.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -3.825001 -24.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -12.025 -24.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -3.825001 -24.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -12.025 -23.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -3.825001 -23.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at -12.025 -23.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at -3.825001 -23.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at -12.025 -22.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at -3.825001 -22.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at -12.025 -22.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at -3.825001 -22.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at -12.025 -21.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at -3.825001 -21.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at -12.025 -21.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -3.825001 -21.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -12.025 -20.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -3.825001 -20.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at -12.025 -20.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at -3.825001 -20.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at -12.025 -19.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at -3.825001 -19.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd roundrect
		(at -12.025 -19.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "58" smd roundrect
		(at -3.825001 -19.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "59" smd roundrect
		(at -12.025 -18.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "60" smd roundrect
		(at -3.825001 -18.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "61" smd roundrect
		(at -12.025 -18.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "62" smd roundrect
		(at -3.825001 -18.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "63" smd roundrect
		(at -12.025 -17.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "64" smd roundrect
		(at -3.825001 -17.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "65" smd roundrect
		(at -12.025 -17.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "66" smd roundrect
		(at -3.825001 -17.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "67" smd roundrect
		(at -12.025 -16.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "68" smd roundrect
		(at -3.825001 -16.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "69" smd roundrect
		(at -12.025 -16.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "70" smd roundrect
		(at -3.825001 -16.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "71" smd roundrect
		(at -12.025 -15.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "72" smd roundrect
		(at -3.825001 -15.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "73" smd roundrect
		(at -12.025 -15.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "74" smd roundrect
		(at -3.825001 -15.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "75" smd roundrect
		(at -12.025 -14.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "76" smd roundrect
		(at -3.825001 -14.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "77" smd roundrect
		(at -12.025 -14.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "78" smd roundrect
		(at -3.825001 -14.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "79" smd roundrect
		(at -12.025 -13.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "80" smd roundrect
		(at -3.825001 -13.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "81" smd roundrect
		(at -12.025 -13.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "82" smd roundrect
		(at -3.825001 -13.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "83" smd roundrect
		(at -12.025 -12.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "84" smd roundrect
		(at -3.825001 -12.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "85" smd roundrect
		(at -12.025 -12.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "86" smd roundrect
		(at -3.825001 -12.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "87" smd roundrect
		(at -12.025 -11.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "88" smd roundrect
		(at -3.825001 -11.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "89" smd roundrect
		(at -12.025 -11.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "90" smd roundrect
		(at -3.825001 -11.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "91" smd roundrect
		(at -12.025 -10.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "92" smd roundrect
		(at -3.825001 -10.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "93" smd roundrect
		(at -12.025 -10.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "94" smd roundrect
		(at -3.825001 -10.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "95" smd roundrect
		(at -12.025 -9.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "96" smd roundrect
		(at -3.825001 -9.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "97" smd roundrect
		(at -12.025 -9.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "98" smd roundrect
		(at -3.825001 -9.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "99" smd roundrect
		(at -12.025 -8.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "100" smd roundrect
		(at -3.825001 -8.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "101" smd roundrect
		(at -12.025 -8.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "102" smd roundrect
		(at -3.825001 -8.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "103" smd roundrect
		(at -12.025 -7.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "104" smd roundrect
		(at -3.825001 -7.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "105" smd roundrect
		(at -12.025 -7.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "106" smd roundrect
		(at -3.825001 -7.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "107" smd roundrect
		(at -12.025 -6.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "108" smd roundrect
		(at -3.825001 -6.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "109" smd roundrect
		(at -12.025 -6.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "110" smd roundrect
		(at -3.825001 -6.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "111" smd roundrect
		(at -12.025 -5.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "112" smd roundrect
		(at -3.825001 -5.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "113" smd roundrect
		(at -12.025 -5.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "114" smd roundrect
		(at -3.825001 -5.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "115" smd roundrect
		(at -12.025 -4.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "116" smd roundrect
		(at -3.825001 -4.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "117" smd roundrect
		(at -12.025 -4.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "118" smd roundrect
		(at -3.825001 -4.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "119" smd roundrect
		(at -12.025 -3.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "120" smd roundrect
		(at -3.825001 -3.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "121" smd roundrect
		(at -12.025 -3.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "122" smd roundrect
		(at -3.825001 -3.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "123" smd roundrect
		(at -12.025 -2.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "124" smd roundrect
		(at -3.825001 -2.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "125" smd roundrect
		(at -12.025 -2.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "126" smd roundrect
		(at -3.825001 -2.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "127" smd roundrect
		(at -12.025 -1.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "128" smd roundrect
		(at -3.825001 -1.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "129" smd roundrect
		(at -12.025 -1.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "130" smd roundrect
		(at -3.825001 -1.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "131" smd roundrect
		(at -12.025 -0.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "132" smd roundrect
		(at -3.825001 -0.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "133" smd roundrect
		(at -12.025 -0.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "134" smd roundrect
		(at -3.825001 -0.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "135" smd roundrect
		(at -12.025 0.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "136" smd roundrect
		(at -3.825001 0.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "137" smd roundrect
		(at -12.025 0.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "138" smd roundrect
		(at -3.825001 0.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "139" smd roundrect
		(at -12.025 1.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "140" smd roundrect
		(at -3.825001 1.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "141" smd roundrect
		(at -12.025 1.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "142" smd roundrect
		(at -3.825001 1.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "143" smd roundrect
		(at -12.025 2.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "144" smd roundrect
		(at -3.825001 2.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "145" smd roundrect
		(at -12.025 4.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "146" smd roundrect
		(at -3.825001 4.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "147" smd roundrect
		(at -12.025 5.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "148" smd roundrect
		(at -3.825001 5.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "149" smd roundrect
		(at -12.025 5.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "150" smd roundrect
		(at -3.825001 5.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "151" smd roundrect
		(at -12.025 6.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "152" smd roundrect
		(at -3.825001 6.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "153" smd roundrect
		(at -12.025 6.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "154" smd roundrect
		(at -3.825001 6.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "155" smd roundrect
		(at -12.025 7.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "156" smd roundrect
		(at -3.825001 7.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "157" smd roundrect
		(at -12.025 7.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "158" smd roundrect
		(at -3.825001 7.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "159" smd roundrect
		(at -12.025 8.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "160" smd roundrect
		(at -3.825001 8.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "161" smd roundrect
		(at -12.025 8.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "162" smd roundrect
		(at -3.825001 8.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "163" smd roundrect
		(at -12.025 9.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "164" smd roundrect
		(at -3.825001 9.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "165" smd roundrect
		(at -12.025 9.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "166" smd roundrect
		(at -3.825001 9.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "167" smd roundrect
		(at -12.025 10.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "168" smd roundrect
		(at -3.825001 10.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "169" smd roundrect
		(at -12.025 10.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "170" smd roundrect
		(at -3.825001 10.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "171" smd roundrect
		(at -12.025 11.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "172" smd roundrect
		(at -3.825001 11.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "173" smd roundrect
		(at -12.025 11.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "174" smd roundrect
		(at -3.825001 11.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "175" smd roundrect
		(at -12.025 12.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "176" smd roundrect
		(at -3.825001 12.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "177" smd roundrect
		(at -12.025 12.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "178" smd roundrect
		(at -3.825001 12.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "179" smd roundrect
		(at -12.025 13.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "180" smd roundrect
		(at -3.825001 13.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "181" smd roundrect
		(at -12.025 13.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "182" smd roundrect
		(at -3.825001 13.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "183" smd roundrect
		(at -12.025 14.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "184" smd roundrect
		(at -3.825001 14.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "185" smd roundrect
		(at -12.025 14.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "186" smd roundrect
		(at -3.825001 14.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "187" smd roundrect
		(at -12.025 15.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "188" smd roundrect
		(at -3.825001 15.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "189" smd roundrect
		(at -12.025 15.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "190" smd roundrect
		(at -3.825001 15.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "191" smd roundrect
		(at -12.025 16.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "192" smd roundrect
		(at -3.825001 16.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "193" smd roundrect
		(at -12.025 16.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "194" smd roundrect
		(at -3.825001 16.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "195" smd roundrect
		(at -12.025 17.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "196" smd roundrect
		(at -3.825001 17.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "197" smd roundrect
		(at -12.025 17.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "198" smd roundrect
		(at -3.825001 17.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "199" smd roundrect
		(at -12.025 18.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "200" smd roundrect
		(at -3.825001 18.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "201" smd roundrect
		(at -12.025 18.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "202" smd roundrect
		(at -3.825001 18.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "203" smd roundrect
		(at -12.025 19.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "204" smd roundrect
		(at -3.825001 19.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "205" smd roundrect
		(at -12.025 19.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "206" smd roundrect
		(at -3.825001 19.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "207" smd roundrect
		(at -12.025 20.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "208" smd roundrect
		(at -3.825001 20.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "209" smd roundrect
		(at -12.025 20.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "210" smd roundrect
		(at -3.825001 20.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "211" smd roundrect
		(at -12.025 21.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "212" smd roundrect
		(at -3.825001 21.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "213" smd roundrect
		(at -12.025 21.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "214" smd roundrect
		(at -3.825001 21.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "215" smd roundrect
		(at -12.025 22.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "216" smd roundrect
		(at -3.825001 22.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "217" smd roundrect
		(at -12.025 22.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "218" smd roundrect
		(at -3.825001 22.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "219" smd roundrect
		(at -12.025 23.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "220" smd roundrect
		(at -3.825001 23.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "221" smd roundrect
		(at -12.025 23.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "222" smd roundrect
		(at -3.825001 23.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "223" smd roundrect
		(at -12.025 24.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "224" smd roundrect
		(at -3.825001 24.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "225" smd roundrect
		(at -12.025 24.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "226" smd roundrect
		(at -3.825001 24.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "227" smd roundrect
		(at -12.025 25.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "228" smd roundrect
		(at -3.825001 25.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "229" smd roundrect
		(at -12.025 25.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "230" smd roundrect
		(at -3.825001 25.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "231" smd roundrect
		(at -12.025 26.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "232" smd roundrect
		(at -3.825001 26.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "233" smd roundrect
		(at -12.025 26.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "234" smd roundrect
		(at -3.825001 26.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "235" smd roundrect
		(at -12.025 27.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "236" smd roundrect
		(at -3.825001 27.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "237" smd roundrect
		(at -12.025 27.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "238" smd roundrect
		(at -3.825001 27.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "239" smd roundrect
		(at -12.025 28.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "240" smd roundrect
		(at -3.825001 28.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "241" smd roundrect
		(at -12.025 28.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "242" smd roundrect
		(at -3.825001 28.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "243" smd roundrect
		(at -12.025 29.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "244" smd roundrect
		(at -3.825001 29.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "245" smd roundrect
		(at -12.025 29.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "246" smd roundrect
		(at -3.825001 29.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "247" smd roundrect
		(at -12.025 30.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "248" smd roundrect
		(at -3.825001 30.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "249" smd roundrect
		(at -12.025 30.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "250" smd roundrect
		(at -3.825001 30.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "251" smd roundrect
		(at -12.025 31.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "252" smd roundrect
		(at -3.825001 31.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "253" smd roundrect
		(at -12.025 31.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "254" smd roundrect
		(at -3.825001 31.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "255" smd roundrect
		(at -12.025 32.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "256" smd roundrect
		(at -3.825001 32.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "257" smd roundrect
		(at -12.025 32.625 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "258" smd roundrect
		(at -3.825001 32.875 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "259" smd roundrect
		(at -12.025 33.125 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "260" smd roundrect
		(at -3.825001 33.375 270)
		(size 0.3 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at 4.075 -33.8 270)
		(size 3.5 4.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07142857143)
	)
	(pad "MP" smd roundrect
		(at 4.075 33.8 270)
		(size 3.5 4.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07142857143)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/SODIMM-260_DDR4_H4.0-5.2_OrientationStd_Socket.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
