(footprint "Samtec_MECF-05-02-L-DV_2x05_P1.27mm_Polarized_Socket_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for 2.4mm PCB's with 05 contacts (polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-05-02-L-DV_2x05_P1.27mm_Polarized_Socket_Horizontal"
		(at 0 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.32 0)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.32 1)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -2.54 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.54 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.27 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.27 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.54 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.54 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/Samtec_MECF-05-02-L-DV_2x05_P1.27mm_Polarized_Socket_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
