(footprint "Samtec_MECF-08-0_-L-DV_2x08_P1.27mm_Polarized_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for PCB's with 08 contacts (polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -5.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-08-0_-L-DV_2x08_P1.27mm_Polarized_Edge"
		(at 0 5.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -6.25 -5)
		(end -5.955 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.955 5)
		(end -5.955 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.955 5)
		(end -2.515 5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.515 -2)
		(end -1.275 -2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.515 5)
		(end -2.515 -2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.275 5)
		(end -1.275 -2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.275 5)
		(end 5.955 5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.955 5)
		(end 5.955 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 6.25 -5)
		(end 5.955 -5)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -4.435 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -4.435 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -3.165 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -3.165 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -0.625 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -0.625 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at 0.645 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at 0.645 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at 1.915 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at 1.915 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at 3.185 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at 3.185 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at 4.455 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at 4.455 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
