(footprint "Samtec_MECF-20-02-NP-L-DV-WT_2x20_P1.27mm_Socket_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for 2.4mm PCB's with 20 contacts (not polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-20-02-NP-L-DV-WT_2x20_P1.27mm_Socket_Horizontal"
		(at 0 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -15.75 0)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" np_thru_hole circle
		(at -13.845 0)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 13.845 1)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" thru_hole circle
		(at 15.75 0)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" smd rect
		(at -12.065 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -12.065 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -10.795 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -10.795 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -9.525 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -9.525 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.255 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.255 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.985 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.985 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -5.715 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -5.715 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -4.445 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -4.445 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -3.175 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -3.175 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.905 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.905 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -0.635 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -0.635 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0.635 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.635 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 1.905 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.905 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 3.175 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 3.175 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 4.445 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 4.445 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 5.715 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 5.715 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 6.985 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 6.985 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 8.255 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 8.255 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 9.525 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 9.525 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 10.795 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 10.795 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 12.065 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 12.065 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/Samtec_MECF-20-02-NP-L-DV-WT_2x20_P1.27mm_Socket_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
