(footprint "Samtec_MECF-30-0_-NP-L-DV_2x30_P1.27mm_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for PCB's with 30 contacts (not polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -5.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-30-0_-NP-L-DV_2x30_P1.27mm_Edge"
		(at 0 5.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -20.25 -5)
		(end -19.925 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -19.925 5)
		(end -19.925 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -19.925 5)
		(end 19.925 5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 19.925 5)
		(end 19.925 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 20.25 -5)
		(end 19.925 -5)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -18.405 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -18.405 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -17.135 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -17.135 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -15.865 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at -15.865 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -14.595 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -14.595 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at -13.325 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at -13.325 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at -12.055 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at -12.055 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at -10.785 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at -10.785 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at -9.515 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at -9.515 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at -8.245 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at -8.245 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at -6.975 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" connect rect
		(at -6.975 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at -5.705 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" connect rect
		(at -5.705 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at -4.435 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" connect rect
		(at -4.435 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at -3.165 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" connect rect
		(at -3.165 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at -1.895 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" connect rect
		(at -1.895 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at -0.625 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" connect rect
		(at -0.625 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at 0.645 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" connect rect
		(at 0.645 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "33" connect rect
		(at 1.915 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at 1.915 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "35" connect rect
		(at 3.185 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at 3.185 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "37" connect rect
		(at 4.455 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at 4.455 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "39" connect rect
		(at 5.725 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at 5.725 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "41" connect rect
		(at 6.995 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at 6.995 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "43" connect rect
		(at 8.265 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at 8.265 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "45" connect rect
		(at 9.535 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at 9.535 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "47" connect rect
		(at 10.805 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at 10.805 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "49" connect rect
		(at 12.075 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at 12.075 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "51" connect rect
		(at 13.345 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" connect rect
		(at 13.345 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "53" connect rect
		(at 14.615 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" connect rect
		(at 14.615 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "55" connect rect
		(at 15.885 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" connect rect
		(at 15.885 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "57" connect rect
		(at 17.155 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" connect rect
		(at 17.155 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "59" connect rect
		(at 18.425 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" connect rect
		(at 18.425 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
