(footprint "Samtec_MECF-60-0_-NP-L-DV_2x60_P1.27mm_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for PCB's with 60 contacts (not polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -5.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-60-0_-NP-L-DV_2x60_P1.27mm_Edge"
		(at 0 5.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -39.25 -5)
		(end -38.975 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -38.975 5)
		(end -38.975 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -38.975 5)
		(end 38.975 5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 38.975 5)
		(end 38.975 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 39.25 -5)
		(end 38.975 -5)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -37.455 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -37.455 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "3" connect rect
		(at -36.185 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "4" connect rect
		(at -36.185 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at -34.915 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at -34.915 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at -33.645 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at -33.645 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at -32.375 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at -32.375 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "11" connect rect
		(at -31.105 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "12" connect rect
		(at -31.105 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "13" connect rect
		(at -29.835 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "14" connect rect
		(at -29.835 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "15" connect rect
		(at -28.565 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "16" connect rect
		(at -28.565 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "17" connect rect
		(at -27.295 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "18" connect rect
		(at -27.295 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "19" connect rect
		(at -26.025 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "20" connect rect
		(at -26.025 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "21" connect rect
		(at -24.755 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "22" connect rect
		(at -24.755 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "23" connect rect
		(at -23.485 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "24" connect rect
		(at -23.485 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "25" connect rect
		(at -22.215 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "26" connect rect
		(at -22.215 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "27" connect rect
		(at -20.945 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "28" connect rect
		(at -20.945 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "29" connect rect
		(at -19.675 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "30" connect rect
		(at -19.675 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "31" connect rect
		(at -18.405 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "32" connect rect
		(at -18.405 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "33" connect rect
		(at -17.135 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "34" connect rect
		(at -17.135 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "35" connect rect
		(at -15.865 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "36" connect rect
		(at -15.865 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "37" connect rect
		(at -14.595 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "38" connect rect
		(at -14.595 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "39" connect rect
		(at -13.325 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "40" connect rect
		(at -13.325 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "41" connect rect
		(at -12.055 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "42" connect rect
		(at -12.055 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "43" connect rect
		(at -10.785 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "44" connect rect
		(at -10.785 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "45" connect rect
		(at -9.515 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "46" connect rect
		(at -9.515 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "47" connect rect
		(at -8.245 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "48" connect rect
		(at -8.245 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "49" connect rect
		(at -6.975 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "50" connect rect
		(at -6.975 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "51" connect rect
		(at -5.705 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "52" connect rect
		(at -5.705 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "53" connect rect
		(at -4.435 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "54" connect rect
		(at -4.435 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "55" connect rect
		(at -3.165 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "56" connect rect
		(at -3.165 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "57" connect rect
		(at -1.895 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "58" connect rect
		(at -1.895 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "59" connect rect
		(at -0.625 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "60" connect rect
		(at -0.625 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "61" connect rect
		(at 0.645 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "62" connect rect
		(at 0.645 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "63" connect rect
		(at 1.915 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "64" connect rect
		(at 1.915 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "65" connect rect
		(at 3.185 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "66" connect rect
		(at 3.185 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "67" connect rect
		(at 4.455 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "68" connect rect
		(at 4.455 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "69" connect rect
		(at 5.725 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "70" connect rect
		(at 5.725 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "71" connect rect
		(at 6.995 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "72" connect rect
		(at 6.995 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "73" connect rect
		(at 8.265 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "74" connect rect
		(at 8.265 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "75" connect rect
		(at 9.535 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "76" connect rect
		(at 9.535 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "77" connect rect
		(at 10.805 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "78" connect rect
		(at 10.805 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "79" connect rect
		(at 12.075 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "80" connect rect
		(at 12.075 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "81" connect rect
		(at 13.345 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "82" connect rect
		(at 13.345 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "83" connect rect
		(at 14.615 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "84" connect rect
		(at 14.615 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "85" connect rect
		(at 15.885 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "86" connect rect
		(at 15.885 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "87" connect rect
		(at 17.155 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "88" connect rect
		(at 17.155 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "89" connect rect
		(at 18.425 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "90" connect rect
		(at 18.425 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "91" connect rect
		(at 19.695 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "92" connect rect
		(at 19.695 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "93" connect rect
		(at 20.965 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "94" connect rect
		(at 20.965 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "95" connect rect
		(at 22.235 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "96" connect rect
		(at 22.235 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "97" connect rect
		(at 23.505 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "98" connect rect
		(at 23.505 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "99" connect rect
		(at 24.775 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "100" connect rect
		(at 24.775 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "101" connect rect
		(at 26.045 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "102" connect rect
		(at 26.045 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "103" connect rect
		(at 27.315 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "104" connect rect
		(at 27.315 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "105" connect rect
		(at 28.585 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "106" connect rect
		(at 28.585 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "107" connect rect
		(at 29.855 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "108" connect rect
		(at 29.855 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "109" connect rect
		(at 31.125 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "110" connect rect
		(at 31.125 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "111" connect rect
		(at 32.395 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "112" connect rect
		(at 32.395 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "113" connect rect
		(at 33.665 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "114" connect rect
		(at 33.665 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "115" connect rect
		(at 34.935 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "116" connect rect
		(at 34.935 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "117" connect rect
		(at 36.205 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "118" connect rect
		(at 36.205 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "119" connect rect
		(at 37.475 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "120" connect rect
		(at 37.475 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
