(footprint "Samtec_MECF-70-02-NP-L-DV_2x70_P1.27mm_Socket_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for 2.4mm PCB's with 70 contacts (not polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-70-02-NP-L-DV_2x70_P1.27mm_Socket_Horizontal"
		(at 0 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -45.595 0)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 45.595 1)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -43.815 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -43.815 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -42.545 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -42.545 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -41.275 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -41.275 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -40.005 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -40.005 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -38.735 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -38.735 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -37.465 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -37.465 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -36.195 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -36.195 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -34.925 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -34.925 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -33.655 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -33.655 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -32.385 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -32.385 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -31.115 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -31.115 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -29.845 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -29.845 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -28.575 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -28.575 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -27.305 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -27.305 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -26.035 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -26.035 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -24.765 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -24.765 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -23.495 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -23.495 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -22.225 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -22.225 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -20.955 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -20.955 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -19.685 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -19.685 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -18.415 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -18.415 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -17.145 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -17.145 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -15.875 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -15.875 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -14.605 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -14.605 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -13.335 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -13.335 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -12.065 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at -12.065 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -10.795 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -10.795 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -9.525 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -9.525 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -8.255 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -8.255 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -6.985 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -6.985 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -5.715 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -5.715 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -4.445 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -4.445 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -3.175 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -3.175 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -1.905 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at -1.905 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at -0.635 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at -0.635 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 0.635 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 0.635 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 1.905 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 1.905 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at 3.175 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at 3.175 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at 4.445 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at 4.445 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at 5.715 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at 5.715 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 6.985 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at 6.985 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at 8.255 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at 8.255 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at 9.525 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 9.525 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at 10.795 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at 10.795 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at 12.065 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at 12.065 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at 13.335 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at 13.335 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at 14.605 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at 14.605 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at 15.875 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at 15.875 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 17.145 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 17.145 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 18.415 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 18.415 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 19.685 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 19.685 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 20.955 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 20.955 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 22.225 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 22.225 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 23.495 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 23.495 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 24.765 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 24.765 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 26.035 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 26.035 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 27.305 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 27.305 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 28.575 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 28.575 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at 29.845 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at 29.845 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at 31.115 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at 31.115 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 32.385 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 32.385 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 33.655 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 33.655 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 34.925 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at 34.925 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at 36.195 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at 36.195 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at 37.465 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at 37.465 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at 38.735 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at 38.735 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 40.005 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 40.005 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at 41.275 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at 41.275 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at 42.545 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at 42.545 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at 43.815 2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at 43.815 -2.3)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/Samtec_MECF-70-02-NP-L-DV_2x70_P1.27mm_Socket_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
