(footprint "molex_EDGELOCK_6-CKT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.molex.com/pdm_docs/sd/2008900106_sd.pdf")
	(tags "Connector PCBEdge molex EDGELOCK")
	(property "Reference" "REF**"
		(at 0 -5.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "molex_EDGELOCK_6-CKT"
		(at 0 17.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -11.95 4)
		(end -11.95 -2.7)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.55 -3.1)
		(end -10.15 -3.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -9.75 -2.7)
		(end -9.75 4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -9.75 4)
		(end -3.55 4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.55 4)
		(end -3.55 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.35 -0.2)
		(end -2.9 -0.2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.7 0)
		(end -2.7 4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -2.7 4)
		(end 2.7 4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.4 -3.9)
		(end -1.4 -1.65)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1 -1.25)
		(end 1 -1.25)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1 -4.3)
		(end -1 -4.3)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.4 -1.65)
		(end 1.4 -3.9)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.7 4)
		(end 2.7 0)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.9 -0.2)
		(end 3.35 -0.2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.55 0)
		(end 3.55 4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.55 4)
		(end 9.75 4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 9.75 4)
		(end 9.75 -2.7)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.15 -3.1)
		(end 10.75 -3.1)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.15 -2.7)
		(end 11.15 4)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -11.95 -2.7)
		(mid -11.832843 -2.982843)
		(end -11.55 -3.1)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -10.15 -3.1)
		(mid -9.867157 -2.982843)
		(end -9.75 -2.7)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -3.55 0)
		(mid -3.491421 -0.141421)
		(end -3.35 -0.2)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -2.9 -0.2)
		(mid -2.758579 -0.141421)
		(end -2.7 0)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -1.4 -3.9)
		(mid -1.282843 -4.182843)
		(end -1 -4.3)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -1 -1.25)
		(mid -1.282843 -1.367157)
		(end -1.4 -1.65)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 1 -4.3)
		(mid 1.282843 -4.182843)
		(end 1.4 -3.9)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 1.4 -1.65)
		(mid 1.282843 -1.367157)
		(end 1 -1.25)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 2.7 0)
		(mid 2.758579 -0.141421)
		(end 2.9 -0.2)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 3.35 -0.2)
		(mid 3.491421 -0.141421)
		(end 3.55 0)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 9.75 -2.7)
		(mid 9.867157 -2.982843)
		(end 10.15 -3.1)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 10.75 -3.1)
		(mid 11.032843 -2.982843)
		(end 11.15 -2.7)
		(layer "Edge.Cuts")
	)
	(fp_text user "Chamfer 30 degree 0.5 mm"
		(at 0 4.7 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" connect roundrect
		(at -8.65 0)
		(size 1 6.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
	)
	(pad "2" connect roundrect
		(at -6.65 0)
		(size 1 6.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
	)
	(pad "3" connect roundrect
		(at -4.65 0)
		(size 1 6.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
	)
	(pad "4" connect roundrect
		(at 4.65 0)
		(size 1 6.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
	)
	(pad "5" connect roundrect
		(at 6.65 0)
		(size 1 6.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
	)
	(pad "6" connect roundrect
		(at 8.65 0)
		(size 1 6.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PCBEdge.3dshapes/molex_EDGELOCK_6-CKT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
