(footprint "PinHeader_2x27_P1.27mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Through hole angled pin header, 2x27, 1.27mm pitch, 4.0mm pin length, double rows")
	(tags "Through hole angled pin header THT 2x27 1.27mm double row")
	(property "Reference" "REF**"
		(at 3.0675 -1.635 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinHeader_2x27_P1.27mm_Horizontal"
		(at 3.0675 34.655 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.27 16.51 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 1.27 0)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 1.27)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 1.27 1.27)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0 2.54)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 1.27 2.54)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 0 3.81)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 1.27 3.81)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 0 5.08)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 1.27 5.08)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 0 6.35)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 1.27 6.35)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 0 7.62)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 1.27 7.62)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 0 8.89)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 1.27 8.89)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at 0 10.16)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at 1.27 10.16)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at 0 11.43)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at 1.27 11.43)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 0 12.7)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 1.27 12.7)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 0 13.97)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 1.27 13.97)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole oval
		(at 0 15.24)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole oval
		(at 1.27 15.24)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole oval
		(at 0 16.51)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole oval
		(at 1.27 16.51)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole oval
		(at 0 17.78)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole oval
		(at 1.27 17.78)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole oval
		(at 0 19.05)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole oval
		(at 1.27 19.05)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole oval
		(at 0 20.32)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole oval
		(at 1.27 20.32)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" thru_hole oval
		(at 0 21.59)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "36" thru_hole oval
		(at 1.27 21.59)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole oval
		(at 0 22.86)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "38" thru_hole oval
		(at 1.27 22.86)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole oval
		(at 0 24.13)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole oval
		(at 1.27 24.13)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole oval
		(at 0 25.4)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "42" thru_hole oval
		(at 1.27 25.4)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole oval
		(at 0 26.67)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "44" thru_hole oval
		(at 1.27 26.67)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole oval
		(at 0 27.94)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "46" thru_hole oval
		(at 1.27 27.94)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "47" thru_hole oval
		(at 0 29.21)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "48" thru_hole oval
		(at 1.27 29.21)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole oval
		(at 0 30.48)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "50" thru_hole oval
		(at 1.27 30.48)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "51" thru_hole oval
		(at 0 31.75)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "52" thru_hole oval
		(at 1.27 31.75)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "53" thru_hole oval
		(at 0 33.02)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "54" thru_hole oval
		(at 1.27 33.02)
		(size 1 1)
		(drill 0.65)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x27_P1.27mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
