(footprint "PinHeader_2x30_P1.27mm_Vertical_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "surface-mounted straight pin header, 2x30, 1.27mm pitch, double rows")
	(tags "Surface mounted pin header SMD 2x30 1.27mm double row")
	(property "Reference" "REF**"
		(at 0 -20.11 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinHeader_2x30_P1.27mm_Vertical_SMD"
		(at 0 20.11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.95 -18.415)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.95 -18.415)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.95 -17.145)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.95 -17.145)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.95 -15.875)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.95 -15.875)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.95 -14.605)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.95 -14.605)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.95 -13.335)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.95 -13.335)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -1.95 -12.065)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.95 -12.065)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.95 -10.795)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.95 -10.795)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.95 -9.525)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.95 -9.525)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.95 -8.255)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.95 -8.255)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.95 -6.985)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.95 -6.985)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.95 -5.715)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.95 -5.715)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -1.95 -4.445)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.95 -4.445)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.95 -3.175)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.95 -3.175)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.95 -1.905)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.95 -1.905)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -1.95 -0.635)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 1.95 -0.635)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -1.95 0.635)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 1.95 0.635)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -1.95 1.905)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 1.95 1.905)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -1.95 3.175)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 1.95 3.175)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -1.95 4.445)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 1.95 4.445)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -1.95 5.715)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 1.95 5.715)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -1.95 6.985)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 1.95 6.985)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -1.95 8.255)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 1.95 8.255)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -1.95 9.525)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 1.95 9.525)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -1.95 10.795)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 1.95 10.795)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -1.95 12.065)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 1.95 12.065)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -1.95 13.335)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 1.95 13.335)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -1.95 14.605)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 1.95 14.605)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -1.95 15.875)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 1.95 15.875)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -1.95 17.145)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 1.95 17.145)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -1.95 18.415)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 1.95 18.415)
		(size 2.4 0.74)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x30_P1.27mm_Vertical_SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
