(footprint "PinHeader_1x04_P2.00mm_Vertical_SMD_Pin1Right"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "surface-mounted straight pin header, 1x04, 2.00mm pitch, single row, style 2 (pin 1 right)")
	(tags "Surface mounted pin header SMD 1x04 2.00mm single row style2 pin1 right")
	(property "Reference" "REF**"
		(at 0 -5.06 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinHeader_1x04_P2.00mm_Vertical_SMD_Pin1Right"
		(at 0 5.06 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 1.175 -3)
		(size 2.35 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.175 -1)
		(size 2.35 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.175 1)
		(size 2.35 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.175 3)
		(size 2.35 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x04_P2.00mm_Vertical_SMD_Pin1Right.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
