(footprint "PinSocket_1x02_P1.00mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Through hole straight socket strip, 1x02, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated")
	(tags "Through hole socket strip THT 1x02 1.00mm single row")
	(property "Reference" "REF**"
		(at -0.29 -2.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinSocket_1x02_P1.00mm_Vertical"
		(at -0.29 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -0.29 0.5 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 0.85 0.85)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 1)
		(size 0.85 0.85)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_1.00mm.3dshapes/PinSocket_1x02_P1.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
