(footprint "PinSocket_1x25_P1.00mm_Vertical_SMD_Pin1Left"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "surface-mounted straight socket strip, 1x25, 1.00mm pitch, single row, style 1 (pin 1 left) (https://gct.co/files/drawings/bc070.pdf), script generated")
	(tags "Surface mounted socket strip SMD 1x25 1.00mm single row style1 pin1 left")
	(property "Reference" "REF**"
		(at 0 -14.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinSocket_1x25_P1.00mm_Vertical_SMD_Pin1Left"
		(at 0 14.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.975 -12)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.975 -11)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.975 -10)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.975 -9)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.975 -8)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.975 -7)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.975 -6)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.975 -5)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -0.975 -4)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.975 -3)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.975 -2)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0.975 -1)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -0.975 0)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 0.975 1)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.975 2)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 0.975 3)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -0.975 4)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 0.975 5)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -0.975 6)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.975 7)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -0.975 8)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.975 9)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -0.975 10)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0.975 11)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -0.975 12)
		(size 1.95 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_1.00mm.3dshapes/PinSocket_1x25_P1.00mm_Vertical_SMD_Pin1Left.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
