(footprint "PinSocket_2x17_P1.27mm_Vertical_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "surface-mounted straight socket strip, 2x17, 1.27mm pitch, double cols (from Kicad 4.0.7!), script generated")
	(tags "Surface mounted socket strip SMD 2x17 1.27mm double row")
	(property "Reference" "REF**"
		(at 0 -12.295 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinSocket_2x17_P1.27mm_Vertical_SMD"
		(at 0 12.295 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 1.8 -10.16)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.8 -10.16)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.8 -8.89)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.8 -8.89)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.8 -7.62)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.8 -7.62)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.8 -6.35)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1.8 -6.35)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.8 -5.08)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -1.8 -5.08)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.8 -3.81)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -1.8 -3.81)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.8 -2.54)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -1.8 -2.54)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.8 -1.27)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -1.8 -1.27)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 1.8 0)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.8 0)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.8 1.27)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -1.8 1.27)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.8 2.54)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -1.8 2.54)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 1.8 3.81)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -1.8 3.81)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1.8 5.08)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -1.8 5.08)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 1.8 6.35)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -1.8 6.35)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 1.8 7.62)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -1.8 7.62)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 1.8 8.89)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -1.8 8.89)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 1.8 10.16)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -1.8 10.16)
		(size 2.1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_2x17_P1.27mm_Vertical_SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
