(footprint "PinSocket_2x04_P2.00mm_Vertical_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "surface-mounted straight socket strip, 2x04, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated")
	(tags "Surface mounted socket strip SMD 2x04 2.00mm double row")
	(property "Reference" "REF**"
		(at 0 -5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinSocket_2x04_P2.00mm_Vertical_SMD"
		(at 0 5.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 3.125 -3)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.125 -3)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 3.125 -1)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.125 -1)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3.125 1)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.125 1)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.125 3)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.125 3)
		(size 2.75 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_2x04_P2.00mm_Vertical_SMD.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
