(footprint "PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Left"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "surface-mounted straight socket strip, 1x30, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated")
	(tags "Surface mounted socket strip SMD 1x30 2.54mm single row style1 pin1 left")
	(property "Reference" "REF**"
		(at 0 -39.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Left"
		(at 0 39.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.65 -36.83)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.65 -34.29)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.65 -31.75)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.65 -29.21)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.65 -26.67)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.65 -24.13)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.65 -21.59)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.65 -19.05)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -1.65 -16.51)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.65 -13.97)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -1.65 -11.43)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.65 -8.89)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.65 -6.35)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.65 -3.81)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.65 -1.27)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.65 1.27)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.65 3.81)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.65 6.35)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1.65 8.89)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.65 11.43)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -1.65 13.97)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.65 16.51)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -1.65 19.05)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1.65 21.59)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.65 24.13)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.65 26.67)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.65 29.21)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.65 31.75)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -1.65 34.29)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 1.65 36.83)
		(size 1.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Left.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
