(footprint "RJ25_Wayconn_MJEA-660X1_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RJ25 6P6C Socket 90 degrees, https://wayconn.com/wp-content/themes/way/datasheet/MJEA-660X1XXX_RJ25_6P6C_PCB_RA.pdf")
	(tags "RJ12 RJ18 RJ25 jack connector 6P6C")
	(property "Reference" "REF**"
		(at -6.985 -3.175 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ25_Wayconn_MJEA-660X1_Horizontal"
		(at -2.55 12.315 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2.55 4.445 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -8.55 4.84)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.45 4.84)
		(size 2.3 2.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.52 1.52)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.02 2.54)
		(size 1.52 1.52)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -2.04 0)
		(size 1.52 1.52)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -3.06 2.54)
		(size 1.52 1.52)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -4.08 0)
		(size 1.52 1.52)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -5.1 2.54)
		(size 1.52 1.52)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ25_Wayconn_MJEA-660X1_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
