(footprint "RJ45_Amphenol_RJHSE5380-08"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Shielded, https://www.amphenolcanada.com/ProductSearch/drawings/AC/RJHSE538X08.pdf")
	(tags "RJ45 8p8c ethernet cat5")
	(property "Reference" "REF**"
		(at 58.68 -9.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Amphenol_RJHSE5380-08"
		(at 58.68 10.37 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 58.68 -6 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.794 -2.54)
		(size 3.2512 3.2512)
		(drill 3.250001)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 58.674 -2.54)
		(size 3.2512 3.2512)
		(drill 3.2512)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 120.142 -2.54)
		(size 3.2512 3.2512)
		(drill 3.2512)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.016 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.032 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.048 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 4.064 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5.08 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 6.096 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 7.112 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 15.748 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 16.764 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 17.78 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 18.796 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 19.812 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 20.828 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 21.844 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 22.86 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 31.496 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 32.512 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 33.528 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 34.544 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 35.56 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 36.576 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 37.592 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 38.608 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 47.244 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at 48.26 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 49.276 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at 50.292 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 51.308 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole circle
		(at 52.324 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole circle
		(at 53.34 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole circle
		(at 54.356 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 62.992 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 64.008 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" thru_hole circle
		(at 65.024 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "36" thru_hole circle
		(at 66.04 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 67.056 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "38" thru_hole circle
		(at 68.072 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at 69.088 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole circle
		(at 70.104 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 78.74 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "42" thru_hole circle
		(at 79.756 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 80.772 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "44" thru_hole circle
		(at 81.788 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole circle
		(at 82.804 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "46" thru_hole circle
		(at 83.82 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "47" thru_hole circle
		(at 84.836 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "48" thru_hole circle
		(at 85.852 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 94.488 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "50" thru_hole circle
		(at 95.504 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "51" thru_hole circle
		(at 96.52 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "52" thru_hole circle
		(at 97.536 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "53" thru_hole circle
		(at 98.552 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "54" thru_hole circle
		(at 99.568 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "55" thru_hole circle
		(at 100.584 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "56" thru_hole circle
		(at 101.6 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 110.236 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "58" thru_hole circle
		(at 111.252 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "59" thru_hole circle
		(at 112.268 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "60" thru_hole circle
		(at 113.284 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "61" thru_hole circle
		(at 114.3 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "62" thru_hole circle
		(at 115.316 1.778)
		(size 1.4986 1.4986)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "63" thru_hole circle
		(at 116.332 0)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "64" thru_hole circle
		(at 117.348 1.778)
		(size 1.4986 1.4986)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -4.572 0.889)
		(size 2.286 2.286)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 50.8 7.62)
		(size 2.286 2.286)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 66.548 7.62)
		(size 2.286 2.286)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 121.92 0.889)
		(size 2.286 2.286)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Amphenol_RJHSE5380-08.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
