(footprint "RJ45_Bel_SI-60062-F"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX, https://belfuse.com/resources/drawings/magneticsolutions/dr-mag-si-60062-f.pdf")
	(tags "RJ45 Magjack")
	(property "Reference" "REF**"
		(at 4.445 -5.49 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Bel_SI-60062-F"
		(at 4.44 18.23 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 4.445 6.37 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.27 6.35)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.16 6.35)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.27 -2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.81 -2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5.08 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 6.35 -2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.62 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 8.89 -2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L1" thru_hole circle
		(at -2.18 10.41)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 0.36 10.41)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 8.53 10.41)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L4" thru_hole circle
		(at 11.07 10.41)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -3.3 3.3)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 12.19 3.3)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Bel_SI-60062-F.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
