(footprint "RJ45_Bel_V895-1001-AW_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 Port RJ45 Magjack Vertical Connector SMD 10/100 Base-T, https://www.belfuse.com/resources/drawings/magneticsolutions/dr-mag-v895-1001-aw.pdf")
	(tags "RJ45 Magjack")
	(property "Reference" "REF**"
		(at -7.8 -10.7 90)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Bel_V895-1001-AW_Vertical"
		(at 0 11.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.715 2.99)
		(size 3.17 3.17)
		(drill 3.17)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.715 2.99)
		(size 3.17 3.17)
		(drill 3.17)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -6.345 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -5.075 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -3.805 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -2.535 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at -1.265 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 0.005 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 2.545 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 3.815 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at 5.085 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 6.355 -10.34)
		(size 0.56 2.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd roundrect
		(at -6.475 -0.665)
		(size 2.41 2.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1037344398)
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd roundrect
		(at -4.585 9.045)
		(size 4.34 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1037344398)
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd roundrect
		(at 4.585 9.045)
		(size 4.34 2.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1037344398)
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd roundrect
		(at 6.475 -0.665)
		(size 2.41 2.79)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1037344398)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Bel_V895-1001-AW_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
