(footprint "RJ45_Connfly_DS1128-09-S8xx-S_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 Port RJ45 8p8c receptacle, shielded, through hole, 2 LEDs, tab up, http://en.connfly.group/static/upload/file//DS1128-09.pdf")
	(tags "RJ45 8p8c ethernet")
	(property "Reference" "REF**"
		(at 13 5.5 270)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Connfly_DS1128-09-S8xx-S_Horizontal"
		(at 3.57 9 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.57 -0.065 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.78 -2.54 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 9.92 -2.54 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1666666667)
	)
	(pad "2" thru_hole circle
		(at 1.02 1.78 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.04 0 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.06 1.78 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 4.08 0 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5.1 1.78 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 6.12 0 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 7.14 1.78 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -3.29 6.6 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at -1 6.6 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 8.14 6.6 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 10.43 6.6 180)
		(size 1.5 1.5)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -4.56 1.02 180)
		(size 2.7 2.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 11.7 1.02 180)
		(size 2.7 2.7)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Connfly_DS1128-09-S8xx-S_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
