(footprint "RJ45_Kycon_G7LX-A88S7-BP-xx_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10/100Base-T RJ45 ethernet magnetic transformer connector horizontal with green/yellow LEDs http://www.kycon.com/Pub_Eng_Draw/G7LX-A88S7-BP-GY.pdf")
	(tags "RJ45 ethernet magnetic")
	(property "Reference" "REF**"
		(at 0 -5.08 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Kycon_G7LX-A88S7-BP-xx_Horizontal"
		(at 7 15.24 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.5 4 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 8.89 -1.27 90)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 8.89 10.16 90)
		(size 3.2 3.2)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.155)
	)
	(pad "2" thru_hole circle
		(at 2.54 1.27 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 2.54 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.54 3.81 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 5.08 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 2.54 6.35 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 7.62 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 2.54 8.89 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.54 -1.27 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0 10.16 90)
		(size 1.6 1.6)
		(drill 0.89)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 13.46 -2.28 90)
		(size 1.72 1.72)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 11.43 -2.28 90)
		(size 1.72 1.72)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 13.46 11.17 90)
		(size 1.72 1.72)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 11.43 11.17 90)
		(size 1.72 1.72)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 5.84 -3.43 90)
		(size 2.2 2.2)
		(drill 1.63)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 5.84 12.32 90)
		(size 2.2 2.2)
		(drill 1.63)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Kycon_G7LX-A88S7-BP-xx_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
