(footprint "RJ45_Molex_0855135013_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 Port, RJ45, Series 85513, vertical, SMD, https://www.molex.com/pdm_docs/sd/855135013_sd.pdf")
	(tags "RJ45 Vertical")
	(property "Reference" "REF**"
		(at 0 -11.89 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Molex_0855135013_Vertical"
		(at 0 12 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.445 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.175 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.905 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.635 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.635 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.905 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.175 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.445 -7.84 180)
		(size 0.76 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L" smd rect
		(at 0 8.09 180)
		(size 8.8 4.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Molex_0855135013_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
