(footprint "RJ45_Pulse_JXD6-0001NL_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RJ45 ethernet transformer with magnetics (https://productfinder.pulseeng.com/doc_type/WEB301/doc_num/JXD6-0001NL/doc_part/JXD6-0001NL.pdf)")
	(tags "ethernet 8p8c transformer magjack")
	(property "Reference" "REF**"
		(at 0 -9.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Pulse_JXD6-0001NL_Horizontal"
		(at 0 9.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0.775 -5.715)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0.775 5.715)
		(size 3 3)
		(drill 3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -11.875 -5.715)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -11.875 -4.445)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -11.875 -3.175)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -11.875 -1.905)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -11.875 -0.635)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -11.875 0.635)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -11.875 1.905)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -11.875 3.175)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -11.875 4.445)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -11.875 5.715)
		(size 3.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at 5.275 -6.77)
		(size 4.6 3.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" smd roundrect
		(at 5.275 6.77)
		(size 4.6 3.26)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Pulse_JXD6-0001NL_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
