(footprint "RJ45_UDE_RB1-125B8G1A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 Port RJ45 Connector Through Hole 10/100/1000 Base-T, https://datasheet.lcsc.com/szlcsc/1901091107_UDE-Corp-RB1-125B8G1A_C363353.pdf#page=3")
	(tags "RJ45 ethernet")
	(property "Reference" "REF**"
		(at 6 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_UDE_RB1-125B8G1A"
		(at 5.5 21 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6 6 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 8.89)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 11.43 8.89)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "L1" thru_hole circle
		(at 12.04 12.27)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L2" thru_hole circle
		(at 9.5 13.79)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L3" thru_hole circle
		(at 1.93 12.27)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "L4" thru_hole circle
		(at -0.61 13.79)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R1" thru_hole rect
		(at 0 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R2" thru_hole circle
		(at 1.27 2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R3" thru_hole circle
		(at 2.54 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R4" thru_hole circle
		(at 3.81 2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R5" thru_hole circle
		(at 5.08 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R6" thru_hole circle
		(at 6.35 2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R7" thru_hole circle
		(at 7.62 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R8" thru_hole circle
		(at 8.89 2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R9" thru_hole circle
		(at 10.16 0)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "R10" thru_hole circle
		(at 11.43 2.54)
		(size 1.9 1.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -2.06 5.84)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 13.49 5.84)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_UDE_RB1-125B8G1A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
