(footprint "RJ45_Wuerth_74980111211_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "RJ45 LAN Transformer 10/100BaseT (https://katalog.we-online.de/pbs/datasheet/74980111211.pdf)")
	(tags "lan magnetics transformer")
	(property "Reference" "REF**"
		(at -11 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Wuerth_74980111211_Horizontal"
		(at 0 10 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 7.42 -6.35)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.42 6.35)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -13.27 -6.61)
		(size 4.6 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -13.27 -4.77)
		(size 4.6 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -13.27 -3.57)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -13.27 -2.55)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -13.27 -1.53)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -13.27 -0.51)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -13.27 0.51)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -13.27 1.53)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -13.27 2.55)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -13.27 3.57)
		(size 4.6 0.61)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -13.27 4.77)
		(size 4.6 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -13.27 6.61)
		(size 4.6 0.81)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 7.42 -8.92)
		(size 4.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 7.42 8.92)
		(size 4.9 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Wuerth_74980111211_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
