(footprint "RJ9_Evercom_5301-440xxx_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Evercom 5301-4P4C RJ9 receptacle, unshielded, https://datasheet.lcsc.com/lcsc/2207051802_EVERCOM-5301-4P4C_C3097715.pdf")
	(tags "RJ9 Connector tab down")
	(property "Reference" "REF**"
		(at 1.84 -4.826 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ9_Evercom_5301-440xxx_Horizontal"
		(at 2.078 15.506 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.698 4.966 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -1.91 6.35)
		(size 3.25 3.25)
		(drill 3.2)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.59 6.35)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1388888889)
	)
	(pad "2" thru_hole circle
		(at 1.27 -2.54)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.81 -2.54)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ9_Evercom_5301-440xxx_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
