(footprint "SATA_Amphenol_10029364-001LF_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10029364.pdf")
	(tags "SATA")
	(property "Reference" "REF**"
		(at -0.04064 -9.90624 0)
		(layer "F.SilkS")
	)
	(property "Value" "SATA_Amphenol_10029364-001LF_Horizontal"
		(at -0.00254 4.26696 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -18.4 0.65508)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Mask" "B.Cu")
	)
	(pad "" np_thru_hole circle
		(at 18.4 0.65508)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Mask" "B.Cu")
	)
	(pad "MP" thru_hole circle
		(at -20 -1.14492)
		(size 1.6 1.6)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
	)
	(pad "MP" thru_hole circle
		(at 20 -1.14492)
		(size 1.6 1.6)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "P1" smd rect
		(at 1.905 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd rect
		(at 0.635 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd rect
		(at -0.635 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd rect
		(at -1.905 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd rect
		(at -3.175 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P6" smd rect
		(at -4.445 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P7" smd rect
		(at -5.715 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd rect
		(at -6.985 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd rect
		(at -8.255 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd rect
		(at -9.525 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P11" smd rect
		(at -10.795 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd rect
		(at -12.065 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P13" smd rect
		(at -13.335 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P14" smd rect
		(at -14.605 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P15" smd rect
		(at -15.875 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" smd rect
		(at 15.87 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S2" smd rect
		(at 14.6 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S3" smd rect
		(at 13.33 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S4" smd rect
		(at 12.06 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S5" smd rect
		(at 10.79 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S6" smd rect
		(at 9.52 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S7" smd rect
		(at 8.25 0.99508)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_SATA_SAS.3dshapes/SATA_Amphenol_10029364-001LF_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
