(footprint "Samtec_FMC_ASP-134602-01_10x40_P1.27mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.marutsu.co.jp/contents/shop/marutsu/ds/asp-134602-01.pdf")
	(tags "FMC HPC")
	(property "Reference" "REF**"
		(at 0 -30.02 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_FMC_ASP-134602-01_10x40_P1.27mm_Vertical"
		(at 0 29.27 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.14 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -27.19 90)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.05 27.19 90)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "A1" smd circle
		(at -5.715 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -5.715 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -5.715 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -5.715 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -5.715 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -5.715 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -5.715 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at -5.715 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at -5.715 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -5.715 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at -5.715 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at -5.715 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at -5.715 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at -5.715 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at -5.715 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd circle
		(at -5.715 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd circle
		(at -5.715 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd circle
		(at -5.715 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd circle
		(at -5.715 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at -5.715 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd circle
		(at -5.715 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd circle
		(at -5.715 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at -5.715 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd circle
		(at -5.715 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd circle
		(at -5.715 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd circle
		(at -5.715 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd circle
		(at -5.715 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A28" smd circle
		(at -5.715 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A29" smd circle
		(at -5.715 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A30" smd circle
		(at -5.715 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A31" smd circle
		(at -5.715 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A32" smd circle
		(at -5.715 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A33" smd circle
		(at -5.715 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A34" smd circle
		(at -5.715 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A35" smd circle
		(at -5.715 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A36" smd circle
		(at -5.715 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A37" smd circle
		(at -5.715 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A38" smd circle
		(at -5.715 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A39" smd circle
		(at -5.715 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A40" smd circle
		(at -5.715 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -4.445 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -4.445 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -4.445 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -4.445 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -4.445 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -4.445 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -4.445 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -4.445 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -4.445 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -4.445 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at -4.445 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at -4.445 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at -4.445 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at -4.445 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at -4.445 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at -4.445 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at -4.445 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at -4.445 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at -4.445 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at -4.445 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd circle
		(at -4.445 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd circle
		(at -4.445 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd circle
		(at -4.445 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd circle
		(at -4.445 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B25" smd circle
		(at -4.445 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd circle
		(at -4.445 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B27" smd circle
		(at -4.445 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B28" smd circle
		(at -4.445 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B29" smd circle
		(at -4.445 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B30" smd circle
		(at -4.445 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B31" smd circle
		(at -4.445 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B32" smd circle
		(at -4.445 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B33" smd circle
		(at -4.445 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B34" smd circle
		(at -4.445 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B35" smd circle
		(at -4.445 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B36" smd circle
		(at -4.445 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B37" smd circle
		(at -4.445 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B38" smd circle
		(at -4.445 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B39" smd circle
		(at -4.445 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B40" smd circle
		(at -4.445 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.175 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -3.175 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -3.175 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -3.175 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -3.175 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at -3.175 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at -3.175 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at -3.175 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at -3.175 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at -3.175 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at -3.175 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at -3.175 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at -3.175 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at -3.175 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at -3.175 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C16" smd circle
		(at -3.175 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C17" smd circle
		(at -3.175 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C18" smd circle
		(at -3.175 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at -3.175 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C20" smd circle
		(at -3.175 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C21" smd circle
		(at -3.175 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at -3.175 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C23" smd circle
		(at -3.175 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C24" smd circle
		(at -3.175 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C25" smd circle
		(at -3.175 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C26" smd circle
		(at -3.175 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C27" smd circle
		(at -3.175 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C28" smd circle
		(at -3.175 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C29" smd circle
		(at -3.175 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C30" smd circle
		(at -3.175 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C31" smd circle
		(at -3.175 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C32" smd circle
		(at -3.175 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C33" smd circle
		(at -3.175 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C34" smd circle
		(at -3.175 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C35" smd circle
		(at -3.175 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C36" smd circle
		(at -3.175 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C37" smd circle
		(at -3.175 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C38" smd circle
		(at -3.175 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C39" smd circle
		(at -3.175 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C40" smd circle
		(at -3.175 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -1.905 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -1.905 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -1.905 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -1.905 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -1.905 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -1.905 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -1.905 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at -1.905 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at -1.905 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at -1.905 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -1.905 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at -1.905 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at -1.905 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at -1.905 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at -1.905 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at -1.905 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D17" smd circle
		(at -1.905 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at -1.905 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at -1.905 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at -1.905 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D21" smd circle
		(at -1.905 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D22" smd circle
		(at -1.905 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd circle
		(at -1.905 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D24" smd circle
		(at -1.905 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D25" smd circle
		(at -1.905 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D26" smd circle
		(at -1.905 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D27" smd circle
		(at -1.905 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D28" smd circle
		(at -1.905 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D29" smd circle
		(at -1.905 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D30" smd circle
		(at -1.905 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D31" smd circle
		(at -1.905 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D32" smd circle
		(at -1.905 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D33" smd circle
		(at -1.905 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D34" smd circle
		(at -1.905 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D35" smd circle
		(at -1.905 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D36" smd circle
		(at -1.905 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D37" smd circle
		(at -1.905 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D38" smd circle
		(at -1.905 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D39" smd circle
		(at -1.905 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D40" smd circle
		(at -1.905 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -0.64 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -0.64 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.64 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -0.64 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -0.64 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at -0.64 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at -0.64 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at -0.64 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at -0.64 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at -0.64 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at -0.64 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at -0.64 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at -0.64 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E14" smd circle
		(at -0.64 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E15" smd circle
		(at -0.64 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E16" smd circle
		(at -0.64 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E17" smd circle
		(at -0.64 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E18" smd circle
		(at -0.64 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E19" smd circle
		(at -0.64 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E20" smd circle
		(at -0.64 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E21" smd circle
		(at -0.64 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E22" smd circle
		(at -0.64 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E23" smd circle
		(at -0.64 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E24" smd circle
		(at -0.64 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E25" smd circle
		(at -0.64 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E26" smd circle
		(at -0.64 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E27" smd circle
		(at -0.64 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E28" smd circle
		(at -0.64 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E29" smd circle
		(at -0.64 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E30" smd circle
		(at -0.64 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E31" smd circle
		(at -0.64 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E32" smd circle
		(at -0.64 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E33" smd circle
		(at -0.64 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E34" smd circle
		(at -0.64 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E35" smd circle
		(at -0.64 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E36" smd circle
		(at -0.64 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E37" smd circle
		(at -0.64 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E38" smd circle
		(at -0.64 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E39" smd circle
		(at -0.64 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E40" smd circle
		(at -0.64 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at 0.64 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at 0.64 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at 0.64 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at 0.64 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0.64 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.64 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 0.64 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 0.64 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 0.64 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at 0.64 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at 0.64 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at 0.64 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F13" smd circle
		(at 0.64 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F14" smd circle
		(at 0.64 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F15" smd circle
		(at 0.64 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F16" smd circle
		(at 0.64 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F17" smd circle
		(at 0.64 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F18" smd circle
		(at 0.64 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F19" smd circle
		(at 0.64 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F20" smd circle
		(at 0.64 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F21" smd circle
		(at 0.64 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F22" smd circle
		(at 0.64 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F23" smd circle
		(at 0.64 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F24" smd circle
		(at 0.64 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F25" smd circle
		(at 0.64 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F26" smd circle
		(at 0.64 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F27" smd circle
		(at 0.64 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F28" smd circle
		(at 0.64 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F29" smd circle
		(at 0.64 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F30" smd circle
		(at 0.64 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F31" smd circle
		(at 0.64 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F32" smd circle
		(at 0.64 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F33" smd circle
		(at 0.64 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F34" smd circle
		(at 0.64 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F35" smd circle
		(at 0.64 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F36" smd circle
		(at 0.64 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F37" smd circle
		(at 0.64 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F38" smd circle
		(at 0.64 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F39" smd circle
		(at 0.64 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F40" smd circle
		(at 0.64 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at 1.905 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at 1.905 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at 1.905 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at 1.905 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at 1.905 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at 1.905 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 1.905 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 1.905 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 1.905 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at 1.905 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 1.905 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at 1.905 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G13" smd circle
		(at 1.905 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G14" smd circle
		(at 1.905 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G15" smd circle
		(at 1.905 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G16" smd circle
		(at 1.905 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G17" smd circle
		(at 1.905 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G18" smd circle
		(at 1.905 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G19" smd circle
		(at 1.905 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G20" smd circle
		(at 1.905 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G21" smd circle
		(at 1.905 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G22" smd circle
		(at 1.905 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G23" smd circle
		(at 1.905 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G24" smd circle
		(at 1.905 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G25" smd circle
		(at 1.905 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G26" smd circle
		(at 1.905 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G27" smd circle
		(at 1.905 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G28" smd circle
		(at 1.905 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G29" smd circle
		(at 1.905 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G30" smd circle
		(at 1.905 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G31" smd circle
		(at 1.905 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G32" smd circle
		(at 1.905 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G33" smd circle
		(at 1.905 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G34" smd circle
		(at 1.905 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G35" smd circle
		(at 1.905 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G36" smd circle
		(at 1.905 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G37" smd circle
		(at 1.905 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G38" smd circle
		(at 1.905 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G39" smd circle
		(at 1.905 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G40" smd circle
		(at 1.905 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at 3.175 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at 3.175 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at 3.175 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at 3.175 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at 3.175 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at 3.175 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 3.175 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 3.175 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 3.175 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 3.175 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 3.175 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 3.175 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 3.175 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at 3.175 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H15" smd circle
		(at 3.175 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H16" smd circle
		(at 3.175 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H17" smd circle
		(at 3.175 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H18" smd circle
		(at 3.175 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at 3.175 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at 3.175 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H21" smd circle
		(at 3.175 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H22" smd circle
		(at 3.175 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd circle
		(at 3.175 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H24" smd circle
		(at 3.175 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H25" smd circle
		(at 3.175 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H26" smd circle
		(at 3.175 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H27" smd circle
		(at 3.175 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H28" smd circle
		(at 3.175 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H29" smd circle
		(at 3.175 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H30" smd circle
		(at 3.175 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H31" smd circle
		(at 3.175 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H32" smd circle
		(at 3.175 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H33" smd circle
		(at 3.175 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H34" smd circle
		(at 3.175 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H35" smd circle
		(at 3.175 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H36" smd circle
		(at 3.175 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H37" smd circle
		(at 3.175 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H38" smd circle
		(at 3.175 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H39" smd circle
		(at 3.175 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H40" smd circle
		(at 3.175 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at 4.445 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at 4.445 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at 4.445 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at 4.445 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at 4.445 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at 4.445 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at 4.445 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 4.445 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 4.445 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at 4.445 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 4.445 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 4.445 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at 4.445 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at 4.445 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J15" smd circle
		(at 4.445 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J16" smd circle
		(at 4.445 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J17" smd circle
		(at 4.445 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J18" smd circle
		(at 4.445 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J19" smd circle
		(at 4.445 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J20" smd circle
		(at 4.445 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J21" smd circle
		(at 4.445 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J22" smd circle
		(at 4.445 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J23" smd circle
		(at 4.445 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J24" smd circle
		(at 4.445 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J25" smd circle
		(at 4.445 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J26" smd circle
		(at 4.445 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J27" smd circle
		(at 4.445 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J28" smd circle
		(at 4.445 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J29" smd circle
		(at 4.445 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J30" smd circle
		(at 4.445 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J31" smd circle
		(at 4.445 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J32" smd circle
		(at 4.445 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J33" smd circle
		(at 4.445 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J34" smd circle
		(at 4.445 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J35" smd circle
		(at 4.445 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J36" smd circle
		(at 4.445 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J37" smd circle
		(at 4.445 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J38" smd circle
		(at 4.445 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J39" smd circle
		(at 4.445 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J40" smd circle
		(at 4.445 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at 5.715 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at 5.715 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at 5.715 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at 5.715 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at 5.715 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at 5.715 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at 5.715 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 5.715 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 5.715 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at 5.715 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 5.715 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at 5.715 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at 5.715 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at 5.715 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K15" smd circle
		(at 5.715 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K16" smd circle
		(at 5.715 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K17" smd circle
		(at 5.715 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K18" smd circle
		(at 5.715 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K19" smd circle
		(at 5.715 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K20" smd circle
		(at 5.715 -0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K21" smd circle
		(at 5.715 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K22" smd circle
		(at 5.715 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K23" smd circle
		(at 5.715 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K24" smd circle
		(at 5.715 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K25" smd circle
		(at 5.715 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K26" smd circle
		(at 5.715 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K27" smd circle
		(at 5.715 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K28" smd circle
		(at 5.715 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K29" smd circle
		(at 5.715 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K30" smd circle
		(at 5.715 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K31" smd circle
		(at 5.715 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K32" smd circle
		(at 5.715 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K33" smd circle
		(at 5.715 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K34" smd circle
		(at 5.715 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K35" smd circle
		(at 5.715 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K36" smd circle
		(at 5.715 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K37" smd circle
		(at 5.715 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K38" smd circle
		(at 5.715 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K39" smd circle
		(at 5.715 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K40" smd circle
		(at 5.715 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec.3dshapes/Samtec_FMC_ASP-134602-01_10x40_P1.27mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
