(footprint "Samtec_FMC_ASP-134604-01_4x40_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://suddendocs.samtec.com/prints/asp-134604-01-mkt.pdf")
	(tags "FMC LPC VITA ")
	(property "Reference" "REF**"
		(at -8.5 0 90)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_FMC_ASP-134604-01_4x40_Vertical"
		(at 9 0 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -27.19 90)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.05 27.19 90)
		(size 1.27 1.27)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
	)
	(pad "C01" smd circle
		(at -3.175 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C02" smd circle
		(at -3.175 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C03" smd circle
		(at -3.175 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C04" smd circle
		(at -3.175 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C05" smd circle
		(at -3.175 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C06" smd circle
		(at -3.175 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C07" smd circle
		(at -3.175 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C08" smd circle
		(at -3.175 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C09" smd circle
		(at -3.175 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at -3.175 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at -3.175 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at -3.175 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at -3.175 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at -3.175 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at -3.175 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C16" smd circle
		(at -3.175 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C17" smd circle
		(at -3.175 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C18" smd circle
		(at -3.175 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at -3.175 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C20" smd circle
		(at -3.175 -0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C21" smd circle
		(at -3.175 0.64 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at -3.175 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C23" smd circle
		(at -3.175 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C24" smd circle
		(at -3.175 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C25" smd circle
		(at -3.175 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C26" smd circle
		(at -3.175 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C27" smd circle
		(at -3.175 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C28" smd circle
		(at -3.175 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C29" smd circle
		(at -3.175 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C30" smd circle
		(at -3.175 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C31" smd circle
		(at -3.175 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C32" smd circle
		(at -3.175 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C33" smd circle
		(at -3.175 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C34" smd circle
		(at -3.175 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C35" smd circle
		(at -3.175 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C36" smd circle
		(at -3.175 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C37" smd circle
		(at -3.175 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C38" smd circle
		(at -3.175 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C39" smd circle
		(at -3.175 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C40" smd circle
		(at -3.175 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D01" smd circle
		(at -1.905 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D02" smd circle
		(at -1.905 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D03" smd circle
		(at -1.905 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D04" smd circle
		(at -1.905 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D05" smd circle
		(at -1.905 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D06" smd circle
		(at -1.905 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D07" smd circle
		(at -1.905 -17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D08" smd circle
		(at -1.905 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D09" smd circle
		(at -1.905 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at -1.905 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -1.905 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at -1.905 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at -1.905 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at -1.905 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at -1.905 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at -1.905 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D17" smd circle
		(at -1.905 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at -1.905 -3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at -1.905 -1.91 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at -1.905 -0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D21" smd circle
		(at -1.905 0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D22" smd circle
		(at -1.905 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd circle
		(at -1.905 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D24" smd circle
		(at -1.905 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D25" smd circle
		(at -1.905 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D26" smd circle
		(at -1.905 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D27" smd circle
		(at -1.905 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D28" smd circle
		(at -1.905 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D29" smd circle
		(at -1.905 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D30" smd circle
		(at -1.905 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D31" smd circle
		(at -1.905 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D32" smd circle
		(at -1.905 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D33" smd circle
		(at -1.905 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D34" smd circle
		(at -1.905 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D35" smd circle
		(at -1.905 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D36" smd circle
		(at -1.905 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D37" smd circle
		(at -1.905 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D38" smd circle
		(at -1.905 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D39" smd circle
		(at -1.905 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D40" smd circle
		(at -1.905 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G01" smd circle
		(at 1.905 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G02" smd circle
		(at 1.905 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G03" smd circle
		(at 1.905 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G04" smd circle
		(at 1.905 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G05" smd circle
		(at 1.905 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G06" smd circle
		(at 1.905 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G07" smd circle
		(at 1.905 -17.14 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G08" smd circle
		(at 1.905 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G09" smd circle
		(at 1.905 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at 1.905 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 1.905 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at 1.905 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G13" smd circle
		(at 1.905 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G14" smd circle
		(at 1.905 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G15" smd circle
		(at 1.905 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G16" smd circle
		(at 1.905 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G17" smd circle
		(at 1.905 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G18" smd circle
		(at 1.905 -3.17 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G19" smd circle
		(at 1.905 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G20" smd circle
		(at 1.905 -0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G21" smd circle
		(at 1.905 0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G22" smd circle
		(at 1.905 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G23" smd circle
		(at 1.905 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G24" smd circle
		(at 1.905 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G25" smd circle
		(at 1.905 5.71 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G26" smd circle
		(at 1.905 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G27" smd circle
		(at 1.905 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G28" smd circle
		(at 1.905 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G29" smd circle
		(at 1.905 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G30" smd circle
		(at 1.905 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G31" smd circle
		(at 1.905 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G32" smd circle
		(at 1.905 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G33" smd circle
		(at 1.905 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G34" smd circle
		(at 1.905 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G35" smd circle
		(at 1.905 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G36" smd circle
		(at 1.905 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G37" smd circle
		(at 1.905 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G38" smd circle
		(at 1.905 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G39" smd circle
		(at 1.905 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G40" smd circle
		(at 1.905 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H01" smd circle
		(at 3.175 -24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H02" smd circle
		(at 3.175 -23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H03" smd circle
		(at 3.175 -22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H04" smd circle
		(at 3.175 -20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H05" smd circle
		(at 3.175 -19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H06" smd circle
		(at 3.175 -18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H07" smd circle
		(at 3.175 -17.14 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H08" smd circle
		(at 3.175 -15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H09" smd circle
		(at 3.175 -14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 3.175 -13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 3.175 -12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 3.175 -10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 3.175 -9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at 3.175 -8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H15" smd circle
		(at 3.175 -6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H16" smd circle
		(at 3.175 -5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H17" smd circle
		(at 3.175 -4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H18" smd circle
		(at 3.175 -3.17 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at 3.175 -1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at 3.175 -0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H21" smd circle
		(at 3.175 0.635 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H22" smd circle
		(at 3.175 1.905 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd circle
		(at 3.175 3.175 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H24" smd circle
		(at 3.175 4.445 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H25" smd circle
		(at 3.175 5.715 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H26" smd circle
		(at 3.175 6.985 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H27" smd circle
		(at 3.175 8.255 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H28" smd circle
		(at 3.175 9.525 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H29" smd circle
		(at 3.175 10.795 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H30" smd circle
		(at 3.175 12.065 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H31" smd circle
		(at 3.175 13.335 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H32" smd circle
		(at 3.175 14.605 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H33" smd circle
		(at 3.175 15.875 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H34" smd circle
		(at 3.175 17.145 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H35" smd circle
		(at 3.175 18.415 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H36" smd circle
		(at 3.175 19.685 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H37" smd circle
		(at 3.175 20.955 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H38" smd circle
		(at 3.175 22.225 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H39" smd circle
		(at 3.175 23.495 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H40" smd circle
		(at 3.175 24.765 90)
		(size 0.64 0.64)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec.3dshapes/Samtec_FMC_ASP-134604-01_4x40_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
