(footprint "Samtec_HLE-114-02-xxx-DV-BE-LC_2x14_P2.54mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-114-02-xxx-DV-BE-LC, 14 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
	(tags "connector Samtec HLE horizontal")
	(property "Reference" "REF**"
		(at 0 -4.76 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HLE-114-02-xxx-DV-BE-LC_2x14_P2.54mm_Horizontal"
		(at 0 4.76 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.84 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -16.51 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -16.51 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -15.24 0)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -13.97 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -13.97 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -11.43 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -11.43 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.89 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.89 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -6.35 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -6.35 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -3.81 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -3.81 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -1.27 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.81 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.81 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.35 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.35 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 8.89 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 8.89 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 11.43 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 11.43 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 13.97 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 13.97 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.24 0)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 16.51 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 16.51 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -16.51 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -16.51 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -13.97 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -13.97 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -11.43 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -11.43 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.89 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.89 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.35 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.35 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.81 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.81 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.27 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -1.27 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.27 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.27 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 3.81 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 3.81 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 6.35 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 6.35 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 8.89 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 8.89 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 11.43 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 11.43 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 13.97 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 13.97 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 16.51 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 16.51 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-114-02-xxx-DV-LC_2x14_P2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
