(footprint "Samtec_HLE-133-02-xxx-DV-BE-LC_2x33_P2.54mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-133-02-xxx-DV-BE-LC, 33 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
	(tags "connector Samtec HLE horizontal")
	(property "Reference" "REF**"
		(at 0 -4.76 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HLE-133-02-xxx-DV-BE-LC_2x33_P2.54mm_Horizontal"
		(at 0 4.76 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.84 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -40.64 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -40.64 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -39.37 0)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -38.1 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -38.1 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -35.56 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -35.56 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -33.02 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -33.02 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -30.48 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -30.48 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -27.94 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -27.94 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -25.4 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -25.4 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -22.86 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -22.86 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -20.32 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -20.32 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -17.78 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -17.78 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -15.24 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -15.24 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -12.7 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -12.7 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -10.16 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -10.16 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.62 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.62 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5.08 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -5.08 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -2.54 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -2.54 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.08 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.08 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.16 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.16 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.7 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.7 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.24 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.24 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 17.78 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 17.78 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 20.32 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 20.32 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 22.86 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 22.86 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 25.4 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 25.4 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.94 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.94 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 30.48 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 30.48 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 33.02 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 33.02 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 35.56 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 35.56 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 38.1 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 38.1 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 39.37 0)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 40.64 -1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 40.64 1.27)
		(size 0.97 0.97)
		(drill 0.97)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -40.64 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -40.64 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -38.1 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -38.1 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -35.56 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -35.56 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -33.02 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -33.02 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -30.48 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -30.48 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -27.94 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -27.94 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -25.4 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -25.4 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -22.86 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -22.86 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -20.32 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -20.32 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -17.78 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -17.78 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -15.24 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -15.24 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -12.7 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -12.7 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -10.16 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -10.16 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -7.62 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -7.62 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -5.08 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -5.08 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -2.54 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -2.54 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 0 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 0 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 2.54 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 2.54 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 5.08 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 5.08 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 7.62 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 7.62 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 10.16 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 10.16 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 12.7 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 12.7 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 15.24 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 15.24 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 17.78 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 17.78 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 20.32 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 20.32 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 22.86 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 22.86 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 25.4 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 25.4 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 27.94 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 27.94 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 30.48 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 30.48 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 33.02 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 33.02 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 35.56 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at 35.56 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at 38.1 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at 38.1 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 40.64 -2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at 40.64 2.72)
		(size 1.27 1.68)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-133-02-xxx-DV-LC_2x33_P2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
