(footprint "Samtec_HLE-104-02-xx-DV-PE-LC_2x04_P2.54mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-104-02-xx-DV-PE-LC, 4 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xx-dv-xe-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-thru.pdf), generated with kicad-footprint-generator")
	(tags "connector Samtec HLE top entry")
	(property "Reference" "REF**"
		(at 3.81 -1.86 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HLE-104-02-xx-DV-PE-LC_2x04_P2.54mm_Horizontal"
		(at 3.81 9.48 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.81 5.65 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 3.81)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.08 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.08 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.35 3.81)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.19084)
	)
	(pad "2" thru_hole circle
		(at 0 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.54 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5.08 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5.08 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.62 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 7.62 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HLE_THT.3dshapes/Samtec_HLE-104-02-xx-DV-PE-LC_2x04_P2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
