(footprint "Samtec_HLE-142-02-xx-DV-PE-LC_2x42_P2.54mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-142-02-xx-DV-PE-LC, 42 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xx-dv-xe-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-thru.pdf), generated with kicad-footprint-generator")
	(tags "connector Samtec HLE top entry")
	(property "Reference" "REF**"
		(at 52.07 -1.86 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HLE-142-02-xx-DV-PE-LC_2x42_P2.54mm_Horizontal"
		(at 52.07 9.48 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 52.07 5.65 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.27 3.81)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.54 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.08 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.08 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.62 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.16 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 10.16 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.7 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 12.7 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.24 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 15.24 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 17.78 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 17.78 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 20.32 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 20.32 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 22.86 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 22.86 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 25.4 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 25.4 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.94 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 27.94 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 30.48 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 30.48 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 33.02 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 33.02 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 35.56 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 35.56 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 38.1 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 38.1 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 40.64 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 40.64 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 43.18 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 43.18 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 45.72 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 45.72 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 48.26 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 48.26 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 50.8 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 50.8 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 53.34 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 53.34 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 55.88 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 55.88 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 58.42 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 58.42 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 60.96 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 60.96 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 63.5 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 63.5 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 66.04 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 66.04 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 68.58 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 68.58 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 71.12 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 71.12 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 73.66 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 73.66 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 76.2 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 76.2 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 78.74 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 78.74 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 81.28 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 81.28 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 83.82 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 83.82 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 86.36 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 86.36 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 88.9 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 88.9 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 91.44 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 91.44 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 93.98 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 93.98 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 96.52 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 96.52 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 99.06 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 99.06 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 101.6 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 101.6 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 102.87 3.81)
		(size 1.19 1.19)
		(drill 1.19)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 104.14 2.54)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 104.14 5.08)
		(size 1.4 1.4)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.19084)
	)
	(pad "2" thru_hole circle
		(at 0 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.54 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5.08 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 5.08 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.62 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 7.62 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 10.16 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 10.16 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 12.7 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 12.7 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 15.24 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 15.24 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 17.78 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 17.78 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 20.32 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 20.32 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 22.86 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 22.86 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 25.4 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 25.4 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole circle
		(at 27.94 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 27.94 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole circle
		(at 30.48 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole circle
		(at 30.48 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole circle
		(at 33.02 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole circle
		(at 33.02 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "29" thru_hole circle
		(at 35.56 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "30" thru_hole circle
		(at 35.56 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "31" thru_hole circle
		(at 38.1 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "32" thru_hole circle
		(at 38.1 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "33" thru_hole circle
		(at 40.64 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "34" thru_hole circle
		(at 40.64 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "35" thru_hole circle
		(at 43.18 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "36" thru_hole circle
		(at 43.18 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "37" thru_hole circle
		(at 45.72 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "38" thru_hole circle
		(at 45.72 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at 48.26 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "40" thru_hole circle
		(at 48.26 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "41" thru_hole circle
		(at 50.8 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "42" thru_hole circle
		(at 50.8 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 53.34 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "44" thru_hole circle
		(at 53.34 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "45" thru_hole circle
		(at 55.88 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "46" thru_hole circle
		(at 55.88 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "47" thru_hole circle
		(at 58.42 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "48" thru_hole circle
		(at 58.42 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "49" thru_hole circle
		(at 60.96 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "50" thru_hole circle
		(at 60.96 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "51" thru_hole circle
		(at 63.5 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "52" thru_hole circle
		(at 63.5 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "53" thru_hole circle
		(at 66.04 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "54" thru_hole circle
		(at 66.04 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "55" thru_hole circle
		(at 68.58 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "56" thru_hole circle
		(at 68.58 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "57" thru_hole circle
		(at 71.12 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "58" thru_hole circle
		(at 71.12 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "59" thru_hole circle
		(at 73.66 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "60" thru_hole circle
		(at 73.66 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "61" thru_hole circle
		(at 76.2 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "62" thru_hole circle
		(at 76.2 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "63" thru_hole circle
		(at 78.74 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "64" thru_hole circle
		(at 78.74 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "65" thru_hole circle
		(at 81.28 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "66" thru_hole circle
		(at 81.28 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "67" thru_hole circle
		(at 83.82 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "68" thru_hole circle
		(at 83.82 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "69" thru_hole circle
		(at 86.36 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "70" thru_hole circle
		(at 86.36 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "71" thru_hole circle
		(at 88.9 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "72" thru_hole circle
		(at 88.9 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "73" thru_hole circle
		(at 91.44 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "74" thru_hole circle
		(at 91.44 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "75" thru_hole circle
		(at 93.98 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "76" thru_hole circle
		(at 93.98 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "77" thru_hole circle
		(at 96.52 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "78" thru_hole circle
		(at 96.52 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "79" thru_hole circle
		(at 99.06 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "80" thru_hole circle
		(at 99.06 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "81" thru_hole circle
		(at 101.6 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "82" thru_hole circle
		(at 101.6 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "83" thru_hole circle
		(at 104.14 0)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "84" thru_hole circle
		(at 104.14 7.62)
		(size 1.31 1.31)
		(drill 0.71)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HLE_THT.3dshapes/Samtec_HLE-142-02-xx-DV-PE-LC_2x42_P2.54mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
