(footprint "Samtec_HPM-15-05-x-S_Straight_1x15_Pitch5.08mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Through hole straight Samtec HPM power header series 3.81mm post length, 1x15, 5.08mm pitch, single row")
	(tags "Through hole Samtec HPM power header series 3.81mm post length THT 1x15 5.08mm single row")
	(property "Reference" "REF**"
		(at 0 -3.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_HPM-15-05-x-S_Straight_1x15_Pitch5.08mm"
		(at 0 74.77 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 35.56 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 5.08)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 10.16)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 15.24)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 20.32)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0 25.4)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 0 30.48)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 0 35.56)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0 40.64)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0 45.72)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 0 50.8)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 0 55.88)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 60.96)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 0 66.04)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 0 71.12)
		(size 2.8 2.8)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Samtec_HPM_THT.3dshapes/Samtec_HPM-15-05-x-S_Straight_1x15_Pitch5.08mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
